O-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## O

OCR_BOTH - Static variable in class com.hsm.barcode.DecoderConfigValues.OCRMode
  OCR Both Video (white & black high)
OCR_INVERSE - Static variable in class com.hsm.barcode.DecoderConfigValues.OCRMode
  OCR Inverse Video (white high)
OCR_NORMAL_VIDEO - Static variable in class com.hsm.barcode.DecoderConfigValues.OCRMode
  OCR Normal Video (black high)
OCR_OFF - Static variable in class com.hsm.barcode.DecoderConfigValues.OCRMode
  OCR Disabled
OFF - Static variable in class com.hsm.barcode.ExposureValues.SpecularExclusion
  Deprecated.
  No specular will be removed.
off(Context) - Method in class com.rscja.deviceapi.ScanerLedLight
  关闭LED灯
  Switch off LED light
On(Context) - Method in class com.rscja.deviceapi.ScanerLedLight
  打开LED灯
  Switch on LED light
onBDSatelliteChanged(ArrayList<SatelliteEntity>) - Method in interface com.rscja.deviceapi.BDNavigation.BDStatusListener
  卫星信息改变时调用
  Call it after satellite infor changed.
onBDSatelliteFIX(int) - Method in interface com.rscja.deviceapi.BDNavigation.BDStatusListener
  定位成功后调用
  Call it after postioning success.
onBDSatelliteLocating() - Method in interface com.rscja.deviceapi.BDNavigation.BDStatusListener
  定位时调用
  Call it when postioning
onBDSatelliteUsedChanged(int) - Method in interface com.rscja.deviceapi.BDNavigation.BDStatusListener
  已用卫星数改变后调用
  Call it after used satellite qty changed.
onBDSatelliteViewChanged(int) - Method in interface com.rscja.deviceapi.BDNavigation.BDStatusListener
  可见卫星数改变后调用
  Call it after visable satellite qty changed.
onBind(Intent) - Method in class com.rscja.deviceapi.service.BTService
onComplete(boolean, byte[], int, int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.EnrollCallBack
  获取完指纹之后被回调
  call-back after fingerprint acquired
onComplete(boolean, byte[], int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.GRABCallBack
  获取完图像之后被回调
  call-back after acquiring image
onComplete(boolean, int, int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.IdentificationCallBack
onComplete(boolean, byte[], int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.PtCaptureCallBack
  获取完指纹模版数据之后被回调
  call-back after fingerprint template data acquired
onComplete(boolean, int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.TemplateVerifyCallBack
onComplete(boolean, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.EnrollCallBack
  获取完指纹之后被回调
  call-back after fingerprint acquired
onComplete(boolean, int, String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.IdentificationCallBack
onComplete(boolean, byte[], int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.PtCaptureCallBack
  获取完指纹模版数据之后被回调
  call-back after fingerprint
onComplete(boolean, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.TemplateVerifyCallBack
onDataResult(String) - Method in interface com.rscja.deviceapi.BDNavigation.BDLocationListener
  模块数据返回时调用
  Call it when module data returned.
onKeepGoingCallback() - Method in interface com.hsm.barcode.DecoderListener
  Handler for listener when a keep going callback occurs
onLocationChanged(BDLocation) - Method in interface com.rscja.deviceapi.BDNavigation.BDLocationListener
  当位置发生改变后被调用
  Call it after current postion changed.
onMultiReadCallback() - Method in interface com.hsm.barcode.DecoderListener
  Handler for listener when a multiple decode result is available.
onPictureTaken(int, int, int, byte[]) - Method in interface com.zebra.adc.decoder.Barcode2DWithSoft.PictureCallback
  得到图片数据
  acquire picture data
onScanComplete(int, int, byte[]) - Method in interface com.zebra.adc.decoder.Barcode2DWithSoft.ScanCallback
onSpeed(double) - Method in interface com.rscja.deviceapi.BDNavigation.BDStatusListener
  时速
  Speed
onUnbind(Intent) - Method in class com.rscja.deviceapi.service.BTService
onVideoFrame(int, int, int, byte[]) - Method in interface com.zebra.adc.decoder.Barcode2DWithSoft.VideoCallback
  得到视频数据(只支持mot扫描头)
open(Context, BarcodeUtility.ModuleType) - Method in class com.barcode.BarcodeUtility
  打开指定功能 Switch on designated function
open(Context) - Method in class com.rscja.deviceapi.Barcode1D
  打开一维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.deviceapi.Barcode1D
  打开一维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.deviceapi.Barcode2D
  打开二维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.deviceapi.BDNavigation
  打开北斗导航模块
  Switch on Beidou navigation module.
open() - Method in class com.rscja.deviceapi.Infrared
  打开红外模块,默认1200波特率
  Switch on infared module, default 1200 baud rate
open(int) - Method in class com.rscja.deviceapi.Infrared
  打开红外模块
  Switch on infared module
open(int, int) - Method in class com.rscja.deviceapi.Infrared
  打开红外模块
  Switch on infared module
open(int, int, int, int) - Method in class com.rscja.deviceapi.Infrared
  打开红外模块
  Switch on infared module
open() - Method in class com.rscja.deviceapi.LedLight
  打开LED灯
  Switch on LED
open(Context) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  打开二维扫描设备
  Switch on 2D scanning device
openAuxiliaryLight(Context) - Method in class com.rscja.deviceapi.ScanerLedLight
  打开扫描辅助灯，目前只支持C70系列
  Switch on scanning light, support C70 series only
openInventoryEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
openKeyboardHelper(Context) - Method in class com.barcode.BarcodeUtility
  打开键盘助手功能总开关 Switch on main function switch of keyboardemulator
openLED() - Method in class com.rscja.deviceapi.Infrared
  打开辅助灯
  Open LED
Optics - Variable in class com.hsm.barcode.ImagerProperties
  Optics of connected engine

A B C D E F G H I K L M N O P R S T U V W X Y