com.rscja.deviceapi

# Package com.rscja.deviceapi

- Interface Summary
  Interface | Description
  --- | ---
  BDNavigation.BDLocationListener | 北斗位置服务的监听接口 Beidou positioning service monitor contact.
  BDNavigation.BDStatusListener | 北斗模块状态监听接口 Beidou module status monitor contact.
  BDNavigation.TestResultRawData | 获取返回的所有数据，此接口用于测试 Acquire all feedback data, the contact is used for testing.
  FingerprintWithFIPS.EnrollCallBack | 采集指纹回调接口 call-back contact for acquiring fingerprint
  FingerprintWithFIPS.GRABCallBack | 指纹图像回调接口 fingerprint image call-back contact
  FingerprintWithFIPS.IdentificationCallBack | 验证指纹的回调接口 call-back contact of verify fingerprint
  FingerprintWithFIPS.PtCaptureCallBack | 获取指纹模版数据回调接口 Acquire call-back contact fingerprint template data
  FingerprintWithFIPS.TemplateVerifyCallBack | 指纹模版比对 fingerprint template comparison
  FingerprintWithMorpho.EnrollCallBack | 采集指纹回调接口 acquire fingerprint call-back contact
  FingerprintWithMorpho.IdentificationCallBack | 验证指纹的回调接口 call-back contact for fingerprint verification
  FingerprintWithMorpho.PtCaptureCallBack | 设置获取指纹模版回调接口 setup fingerprint template acquire call-back contact
  FingerprintWithMorpho.TemplateVerifyCallBack |
  Printer.PrinterStatusCallBack |
  RFIDWithUHFBluetooth.BTStatusCallback | 连接蓝牙的状态值回调
  RFIDWithUHFBluetooth.KeyEventCallback | 接收扫描按键的回调
  RFIDWithUHFBluetooth.ScanBTCallback | 扫描蓝牙设备的回调接口

- Class Summary
  Class | Description
  --- | ---
  Barcode1D | 一维条码操作类 1D barcode operation class
  Barcode2D | 二维条码操作类 2D barcode operation class.
  BDNavigation | 北斗导航模块操作类
  BuildConfig |
  CardWithBYL | 白玉兰公交卡操作类
  DeviceConfiguration | 设备参数配置类 Device parameter config type
  Fingerprint | 指纹识别模块操作类, Fingerprint identify module operation type
  FingerprintWithFIPS | FIPS指纹识别模块操作类, FIPS fingerprint indentify module operation type,
  FingerprintWithMorpho |
  Infrared | 红外模块操作类 Infared module operation type
  LedLight | 手柄LED灯控制类 Handdeld LED control type
  Module | 自定义模块操作类，用于客户自定义模块 Customed module operation type, used for client customed module
  Printer |
  PSAM | PSAM操作类 PSAM operation type
  RFIDWithISO14443A | RFID模块ISO14443A协议操作类 RFID module ISO 14443A protocol operation type
  RFIDWithISO14443A4CPU | RFID模块ISO14443A CPU卡协议操作类 RFID module ISO14443A CPU card protocol operation type
  RFIDWithISO14443B | RFID模块ISO14443B协议操作类 RFID module ISO14443B protocol operation type
  RFIDWithISO15693 | RFID模块ISO15693协议操作类, RFID module ISO15639 protocol operation type
  RFIDWithLF | RFID低频（125K）操作类 RFID LF (125K) operation type
  RFIDWithUHF | UHF模块操作类 UHF module operation type
  RFIDWithUHF706 | UHF 706所模块操作类
  RFIDWithUHFBluetooth |
  ScanerLedLight | 扫描LED灯控制类（仅C6000有效） Scanning LED light control type ( valid for C6000 only)
  VersionInfo | jar包信息类 jar pack infor type

- Enum Summary
  Enum | Description
  --- | ---
  BDNavigation.BDProviderEnum | 导航类型枚举 Navigation type enum.
  BDNavigation.BDStartModeEnum | 模块启动类型枚举 Module start type enum.
  Fingerprint.BufferEnum | 模块缓冲区枚举 Module buffer zone example.
  FingerprintWithFIPS.DataFormat | 指纹数据格式 Fingerprint data format
  Printer.BarcodeType | 1D条码类型
  Printer.PrinterStatus |
  RFIDWithISO14443A.DESFireEncryptionTypekEnum | DESFire卡加密类型 DESFire card encyption type
  RFIDWithISO14443A.DESFireFileTypekEnum | DESFire卡文件类型 DESFire card file typr
  RFIDWithISO14443A.KeyType | 密钥类型，适用于S50和S70标签。 key type, used for S50 and S70 tags.
  RFIDWithISO14443A.TagType | M1标签类型定义 M1 tag type definition
  RFIDWithISO15693.TagType | 标签类型 Tag type
  RFIDWithUHF.BankEnum | 存储区 Storage
  RFIDWithUHF.LockModeEnum | Deprecated
  RFIDWithUHF.SingleModeEnum | 读取模式 Read mode
  RFIDWithUHFBluetooth.BankEnum | 存储区 Storage
  RFIDWithUHFBluetooth.StatusEnum | 蓝牙状态枚举 CONNECTED:已经连接 DISCONNECTED:已经断开 CONNECTING:连接中