W-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## W

waitForDecode(int) - Method in class com.hsm.barcode.Decoder
  Method used to start decoding.
waitForDecodeTwo(int, DecodeResult) - Method in class com.hsm.barcode.Decoder
  Method to start decoding.
waitMultipleDecode(int) - Method in class com.hsm.barcode.Decoder
  This function is used to read multiple symbols using a single function call.
Width - Variable in class com.hsm.barcode.IQImagingProperties
  Width of image in IntellBarcodeUnits (Practical range -500 to 500)
wIndex - Static variable in class com.rscja.deviceapi.RFIDWithUHFBluetooth
wIndexTAG - Static variable in class com.rscja.deviceapi.RFIDWithUHFBluetooth
write(String, RFIDWithISO14443A.KeyType, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  写卡，此函数包括寻卡和密钥验证异常
  Card writing, this formula includes card searching and key verification err
write(int, String) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  写卡，适用于Urltra light标签
  Card writing, used for Urltra light tag
write(int, String) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  写卡
  card writing
write(int, int, String) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  写卡
  card writing
writeAFI(int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  写入AFI
  Write AFi
writeCameraState(int) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  写入camera状态
  write in camera status
writeData(byte[]) - Method in class com.rscja.deviceapi.BDNavigation
writeData(String, RFIDWithUHF.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
writeData(String, RFIDWithUHF.BankEnum, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
writeData(String, RFIDWithUHF.BankEnum, int, int, String, RFIDWithUHF.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  向标签写入数据
  Write data
writeData(String, RFIDWithUHFBluetooth.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  向标签写入数据
writeData(String, RFIDWithUHFBluetooth.BankEnum, int, int, String, RFIDWithUHFBluetooth.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  向标签写入数据
writeData_Ex(String, RFIDWithUHF.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  向标签写入数据。芯联模块只写EPC数据
  Write data in tag.
writeDataWith4305Card(int, String) - Method in class com.rscja.deviceapi.RFIDWithLF
  写4305卡的某一页（0~31）数据
  write data in card 4305 at random page (0-31)
writeDataWithHitagS(int, String) - Method in class com.rscja.deviceapi.RFIDWithLF
  写Hitag S卡中的某一页的数据
  Write data of random page in Hitag S card
writeDataWithQT(String, RFIDWithUHF.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
writeDataWithQT(String, RFIDWithUHF.BankEnum, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
writeDataWithQT(String, RFIDWithUHF.BankEnum, int, int, String, RFIDWithUHF.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  向标签写入数据 ,用于R2000 QT标签
  write data in tag , used for R2000 QT tag
writeDataWithQT_Ex(String, RFIDWithUHF.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  向标签写入数据,用于R2000 QT标签
  write data into tag, used for R2000 QT tag
writeDSFID(int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  写入DSFID
  Write DSFID
writeRXCharacteristic(byte[]) - Method in class com.rscja.deviceapi.service.BTService
writeScannerCameraId(int) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  写入camera id
  write in camera id
writeScannerState(int) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  写入2D软解码扫描头状态
  write in 2D soft decode scanning module status
writeSpecialPart(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  专用指定标签写分区

A B C D E F G H I K L M N O P R S T U V W X Y