Uses of Class com.rscja.deviceapi.exception.ConfigurationException

## Uses of Class
com.rscja.deviceapi.exception.ConfigurationException

- Packages that use ConfigurationException
  Package | Description
  --- | ---
  com.rscja.deviceapi |

- - ### Uses of ConfigurationException in com.rscja.deviceapi

    Methods in com.rscja.deviceapi that throw ConfigurationException
    Modifier and Type | Method and Description
    --- | ---
    `static DeviceConfiguration` | DeviceConfiguration.`builder1DConfiguration()` 创建一维条码配置信息 Create 1D barcode config infor.
    `static DeviceConfiguration` | DeviceConfiguration.`builder2DConfiguration()` 创建二维条码配置信息 Create 2D barcode config infor.
    `static DeviceConfiguration` | DeviceConfiguration.`builderBDConfiguration()` 创建北斗配置信息 Create Beidou config infor.
    `static DeviceConfiguration` | DeviceConfiguration.`builderDefaultConfiguration()`
    `static DeviceConfiguration` | DeviceConfiguration.`builderFingerprintConfiguration()` 创建Fingerprint配置信息 Create Fingerprint config infor.
    `static DeviceConfiguration` | DeviceConfiguration.`builderInfraredConfiguration()` 创建红外配置信息 Create infrared config infor.
    `static DeviceConfiguration` | DeviceConfiguration.`builderLFConfiguration()` 创建低频配置信息 Create LF config infor.
    `static DeviceConfiguration` | DeviceConfiguration.`builderPrinterConfiguration()` 创建打印机配置信息 Create printer config infor.
    `static DeviceConfiguration` | DeviceConfiguration.`builderRFIDConfiguration()` 创建RFID配置信息 Create RFID config infor.
    `static DeviceConfiguration` | DeviceConfiguration.`builderUHFConfiguration()` 创建UHF配置信息 Create UHF config infor.
    `static RFIDWithUHF706` | RFIDWithUHF706.`getInstance()` 获取UHF操作实例
    `static RFIDWithUHF` | RFIDWithUHF.`getInstance()` 获取UHF操作实例 Acquire UHF operation Instance
    `static RFIDWithLF` | RFIDWithLF.`getInstance()` 获取RFID低频操作实例 Acquire RFID LF operation Instance
    `static RFIDWithISO15693` | RFIDWithISO15693.`getInstance()` 获取ISO15693协议操作实例 Acquire ISO15693 protocol operation Instance
    `static RFIDWithISO14443B` | RFIDWithISO14443B.`getInstance()` 获取ISO14443B协议操作实例 Acquire ISO14443B protocol operation Instance
    `static RFIDWithISO14443A4CPU` | RFIDWithISO14443A4CPU.`getInstance()` 获取ISO14443A CPU卡协议操作实例 Acquire ISO14443A CPU card protocol operation example
    `static RFIDWithISO14443A` | RFIDWithISO14443A.`getInstance()` 获取ISO14443A协议操作实例 Acquire ISO14443A protocol operation Instance
    `static Printer` | Printer.`getInstance()` 获取打印机模块操作实例 Acquire printer module operation Instance
    `static Module` | Module.`getInstance()` 获取操作实例 Acquire operation Instance
    `static Infrared` | Infrared.`getInstance()`
    `static FingerprintWithMorpho` | FingerprintWithMorpho.`getInstance()` 获取指纹模块操作实例 acquire fingerprint module operation eample
    `static FingerprintWithFIPS` | FingerprintWithFIPS.`getInstance()` 获取指纹模块操作实例 Acquire fingerprint module operation Instance
    `static Fingerprint` | Fingerprint.`getInstance()` 获取指纹模块操作实例 Acquire fingerprint module operation Instance.
    `static CardWithBYL` | CardWithBYL.`getInstance()` 获取RFID低频操作实例
    `static BDNavigation` | BDNavigation.`getInstance()` 获取北斗导航模块操作实例 Acquire Beidou navigation module operation example.
    `static Barcode2D` | Barcode2D.`getInstance()` 获取二维条码操作实例 * Acquire 2D barcode operation Instance.
    `static Barcode1D` | Barcode1D.`getInstance()` 获取一维条码操作实例 Acquire 1D barcode operation Instance.