M-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## M

M1_ReadData(int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读取指定扇区指定block的数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。
  Read data in specified block of specified sector, used for S50 and S70 tag.
Mask - Variable in class com.hsm.barcode.SymbologyConfig
  Logical OR of valid masks: SYM_MASK_FLAGS, SYM_MASK_MIN_LEN, SYM_MASK_MAX_LEN
match() - Method in class com.rscja.deviceapi.Fingerprint
  对比模板缓冲区1与模板缓冲区2的指纹模板文件
  fingerprint template file of comparison template buffer zone 1 and template buffer zone 2.
MaxLength - Variable in class com.hsm.barcode.SymbologyConfig
  Maximum length for valid barcode string for this symbology
message(Printer.PrinterStatus) - Method in interface com.rscja.deviceapi.Printer.PrinterStatusCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.EnrollCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.GRABCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.IdentificationCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.PtCaptureCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.TemplateVerifyCallBack
messageInfo(String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.EnrollCallBack
messageInfo(String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.IdentificationCallBack
messageInfo(String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.PtCaptureCallBack
messageInfo(String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.TemplateVerifyCallBack
MICRE13B - Static variable in class com.hsm.barcode.DecoderConfigValues.OCRTemplate
  OCR Micre13B Template
MINIMAL - Static variable in class com.hsm.barcode.ExposureValues.SpecularExclusion
  Deprecated.
  Specular will be removed minimally.
MinLength - Variable in class com.hsm.barcode.SymbologyConfig
  Minimum length for valid barcode string for this symbology
MODERATE - Static variable in class com.hsm.barcode.ExposureValues.SpecularExclusion
  Deprecated.
  Specular will be removed moderately.
Module - Class in com.rscja.deviceapi
  自定义模块操作类，用于客户自定义模块
  Customed module operation type, used for client customed module
morphoEraseAllBase() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  删除所有指纹信息
  delete all fingerprint infor
mRFID - Variable in class com.rscja.deviceapi.CardWithBYL
MultiReadCount - Variable in class com.hsm.barcode.DecodeOptions
  Maximum number of barcodes to read in a single image

A B C D E F G H I K L M N O P R S T U V W X Y