G-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## G

GainValue - Variable in class com.hsm.barcode.ImageAttributes
  Gain value applied on last image captured
genChar(Fingerprint.BufferEnum) - Method in class com.rscja.deviceapi.Fingerprint
  生成特征值（存于指定缓存区）
  Generate feature value( save in specified buffer zone)
generateImg(byte[], String) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  生成bmp图片
  Generate bmp
generateLockCode(RFIDWithUHF.LockModeEnum, RFIDWithUHF.LockModeEnum, RFIDWithUHF.LockModeEnum, RFIDWithUHF.LockModeEnum, RFIDWithUHF.LockModeEnum) - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
genericFunction(char, char[], char) - Method in class com.rscja.deviceapi.RFIDWithISO15693
genericFunction_ex(char, char, char[], int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
getAccess() - Method in class com.rscja.deviceapi.RFIDWithUHF706
  获取权限表
getAFI() - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  获取AFI值
  acquire AFI value
getAltitude() - Method in class com.rscja.deviceapi.entity.BDLocation
  海拔
  altitude
getAnimalFlag() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的AnimalFlag
  acquire AnimalFlag of animal tag
getAPIRevision() - Method in class com.hsm.barcode.Decoder
  Retrieves the revision of the API.
getBalance() - Method in class com.rscja.deviceapi.CardWithBYL
  获取余额和有效期
getBarcodeAimID() - Method in class com.hsm.barcode.Decoder
  Gets the Barcode AimID when `Decoder.waitForDecode(int)` succeeds.
getBarcodeAimModifier() - Method in class com.hsm.barcode.Decoder
  Gets the Barcode AimID when `Decoder.waitForDecode(int)` succeeds.
getBarcodeByteData() - Method in class com.hsm.barcode.Decoder
  Gets the Barcode data when `Decoder.waitForDecode(int)` succeeds.
getBarcodeCodeID() - Method in class com.hsm.barcode.Decoder
  Gets the Barcode CodeID when `Decoder.waitForDecode(int)` succeeds.
getBarcodeData() - Method in class com.hsm.barcode.Decoder
  Gets the Barcode Data in string form when `Decoder.waitForDecode(int)` succeeds.
getBarcodeLength() - Method in class com.hsm.barcode.Decoder
  Gets the Barcode length when `Decoder.waitForDecode(int)` succeeds.
getBattery() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  获取电池电量 单位：百分比
getBaudrate() - Method in class com.rscja.deviceapi.DeviceConfiguration
  获取波特率
  Acquire baud rate
getBluetoothMode() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  获取uhf通信方式是否是蓝牙模式
getBTConnectStatus() - Method in class com.rscja.deviceapi.service.BTService
getBytes(char[]) - Static method in class com.rscja.utility.StringUtility
  char类型数组转byte类型数组
getChars(byte[]) - Static method in class com.rscja.utility.StringUtility
  byte类型数组转char类型数组
getCodeTypeList() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  获取蓝牙连接状态
getControlLogicRevision() - Method in class com.hsm.barcode.Decoder
  Retrieves the revision of the Decoder Control Logic.
getCountryID() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的国家代码
  acquire national code of animal tag
getData() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取数据，仅对数据文件类型有效
  acquire data, it is only valid for data file type only
getData() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签数据
  acquire tag data
getDataBlock() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的DataBlock
  acquire DataBlock of animal tag
getDecodeOptions(DecodeOptions) - Method in class com.hsm.barcode.Decoder
  Gets the decode options parameters.
getDecoder() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
getDecoderRevision() - Method in class com.hsm.barcode.Decoder
  Retrieves the revision of the Decoder.
getDecodeWindow(DecodeWindowing.DecodeWindow) - Method in class com.hsm.barcode.Decoder
  Retrieves the decode window parameters.
getDecodeWindowLimits(DecodeWindowing.DecodeWindowLimits) - Method in class com.hsm.barcode.Decoder
  Retrieves the decode window parameter limits.
getDecodeWindowMode() - Method in class com.hsm.barcode.Decoder
  Retrieves the current decode window mode setting
getDecThreadsRevision() - Method in class com.hsm.barcode.Decoder
  Deprecated.
  Retrieves the revision of the Decoder Threading.
getDESFID() - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  获取DESFID值
  acquire DESFID value
getDeviceName() - Method in class com.rscja.deviceapi.DeviceConfiguration
  获取设备名
  Acquire device name
getDevices(BluetoothDevice, int, byte[]) - Method in interface com.rscja.deviceapi.RFIDWithUHFBluetooth.ScanBTCallback
getEncryptionType() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取加密方式
  acquire encryption method
getEngineID() - Method in class com.hsm.barcode.Decoder
  Retrieves the EngineID of the connected Engine.
getEngineSerialNumber() - Method in class com.hsm.barcode.Decoder
  Retrieves the serial number of the connected Engine.
getEngineType() - Method in class com.hsm.barcode.Decoder
  Retrieves the engine type of the connected Engine.
getEPC() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getErrorCode() - Method in exception com.hsm.barcode.DecoderException
  Returns the error code set when an exception occurs.
getErrorMessage(int) - Method in class com.hsm.barcode.Decoder
  Method used to get associated error message with an error code.
getExposureMode() - Method in class com.hsm.barcode.Decoder
  Gets the exposure mode currently set to be used during scanning.
getExposureSettings(int[]) - Method in class com.hsm.barcode.Decoder
  Gets the current exposure settings for the image sensor.
getFileNo() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取文件号
  acquire file number
getFileSize() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取文件大小，仅对数据文件类型有效
  acquire file size, it is valid for data file type only
getFileType() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取文件类型
  acquire file type
getFingersCount() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取模块中采集的指纹数量
  Acquire collected fingerprint amounts in module.
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHF
  读取模块的工作模式
  read module work mode
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  读取模块的工作模式
GetGen2() - Method in class com.rscja.deviceapi.RFIDWithUHF
  [0] target: s0:0 s1:1 s2:2 s3:3 SL:4 [1] action: 0,1,2,3,4,5,6 [2] t: Disable truncation 0, Enable truncation 1 [3] q: 固定Q算法 0, 动态Q算法 1
  [3] q: fixed Q algorithm 0, dynamic Q algorithm 1
  [4] startQ: 0,1,2,3.....15 注意：在固定Q算法下，Q固定为StartQ，忽略MinQ 和 MaxQ
  [4] startQ: 0,1,2,3.....15 note: in fixed algorithm, Q is fixed as StartQ, neglect MinQ and MaxQ
  [5] minQ: 0,1,2,3.....15 [6] maxQ:0,1,2,3......15 [7] dr:0,1 [8] coding:0,1,2,3 [9] p:0,1 [10] sel:0,1,2,3 [11] Session:0,1,2,3 [12] g:0,1 [13] linkFrequency:0,1,2,3,4,5,6,7
getHardwareType() - Method in class com.rscja.deviceapi.RFIDWithUHF
  读取模块类型
  read module type
getHardwareType() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
getHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithLF
  读取硬件版本
  read hardware version
getId() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签ID
  acquire tag ID
getId() - Method in class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
  获取指纹模块ID(十六进制)
  Acquire fingerprint module ID (hex)
getID() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取指纹ID
  Acquire fingerprint ID
getIDAndPowerWithWattmeter() - Method in class com.rscja.deviceapi.Infrared
  获取电表ID和电能值,97标准
  Acquire powermeter ID and energy value, 97 standard
getIDAndPowerWithWattmeter(int) - Method in class com.rscja.deviceapi.Infrared
  获取电表ID和电能值
  Acquire powermeter ID and energy value
getIdBytes() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签ID
  acquire tag ID
getIdData() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取64bit的识别号数据，十六进制表示
  acquire 64bit identification number, hexdecimal
getImage() - Method in class com.rscja.deviceapi.Fingerprint
  获取指纹图像（存于模块图像缓存区）
  Acquire fingerprint image( save in buffer zone of module image)
getImageHeight() - Method in class com.hsm.barcode.Decoder
  Gets the image height of the connected engine.
getImagerProperties(ImagerProperties) - Method in class com.hsm.barcode.Decoder
  Retrieves the imager properties of the connected engine.
getImageWidth() - Method in class com.hsm.barcode.Decoder
  Gets the image width of the connected engine.
getInstance() - Static method in class com.barcode.BarcodeUtility
  获取条码操作实例 Acquire barcode operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.Barcode1D
  获取一维条码操作实例
  Acquire 1D barcode operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.Barcode2D
  获取二维条码操作实例
  * Acquire 2D barcode operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.BDNavigation
  获取北斗导航模块操作实例
  Acquire Beidou navigation module operation example.
getInstance() - Static method in class com.rscja.deviceapi.CardWithBYL
  获取RFID低频操作实例
getInstance() - Static method in class com.rscja.deviceapi.Fingerprint
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance
getInstance() - Static method in class com.rscja.deviceapi.FingerprintWithMorpho
  获取指纹模块操作实例
  acquire fingerprint module operation eample
getInstance() - Static method in class com.rscja.deviceapi.Infrared
getInstance() - Static method in class com.rscja.deviceapi.LedLight
  获取LED灯操作实例
  Acquire LED operation example
getInstance() - Static method in class com.rscja.deviceapi.Module
  获取操作实例
  Acquire operation Instance
getInstance() - Static method in class com.rscja.deviceapi.Printer
  获取打印机模块操作实例
  Acquire printer module operation Instance
getInstance() - Static method in class com.rscja.deviceapi.PSAM
  获取PSAM操作实例
  Acquire PSAM operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO14443A
  获取ISO14443A协议操作实例
  Acquire ISO14443A protocol operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  获取ISO14443A CPU卡协议操作实例
  Acquire ISO14443A CPU card protocol operation example
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO14443B
  获取ISO14443B协议操作实例
  Acquire ISO14443B protocol operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO15693
  获取ISO15693协议操作实例
  Acquire ISO15693 protocol operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithLF
  获取RFID低频操作实例
  Acquire RFID LF operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHF
  获取UHF操作实例
  Acquire UHF operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHF706
  获取UHF操作实例
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
getInstance() - Static method in class com.rscja.deviceapi.ScanerLedLight
  获取LED灯操作实例
  Acquire LED light operation example
getInstance() - Static method in class com.zebra.adc.decoder.Barcode2DWithSoft
  获取二维软解码操作实例
  Acquire 2D soft decode operation example
getIntegerSomeBit(int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  取整数的某一位
  get one place of integer
getInventoryBID() - Method in class com.rscja.deviceapi.RFIDWithUHF
  是否盘存BID(客户定制函数/Customizing)
getIQImage(IQImagingProperties, Bitmap) - Method in class com.hsm.barcode.Decoder
  Retrieves an IQ Image (intelligent imaging)
getKeyboardHelperParam(Context) - Method in class com.barcode.BarcodeUtility
  获取键盘助手状态值,通过action接收数据`BarcodeUtility.ACTION_SCAN_KEYBOARD_HELPER_PARAM_RESPONSE`.(备注：键盘助手v2.2.0.3 之后的版本才支持)
getKeyEvent(int) - Method in interface com.rscja.deviceapi.RFIDWithUHFBluetooth.KeyEventCallback
getLastDecodeTime() - Method in class com.hsm.barcode.Decoder
  Gets the last decode time for a successful decode
getLastImage(ImageAttributes) - Method in class com.hsm.barcode.Decoder
  Retrieves last image sent to the Decoder.
getLastLocation() - Method in class com.rscja.deviceapi.BDNavigation
  获取最后一次定位数据
  Acquire last postion data.
getLastSatelliteUCount() - Method in class com.rscja.deviceapi.BDNavigation
  获取最新已用卫星数
  Acquire latest occupied satellite qty.
getLastsatelliteVCount() - Method in class com.rscja.deviceapi.BDNavigation
  获取最新可视卫星数
  Acquire latest visable satellite qty.
getLastUTCDateTime() - Method in class com.rscja.deviceapi.BDNavigation
  获取最新UTC时间
  Acquire latest UTC time.
getLat() - Method in class com.rscja.deviceapi.entity.BDLocation
  纬度,北纬为正数，南纬为负数
  Lat, north latitude is positive, south latitude is negative
getLightsMode() - Method in class com.hsm.barcode.Decoder
  Retrieves the current lights mode for scanning.
getLon() - Method in class com.rscja.deviceapi.entity.BDLocation
  经度，东经为正数，西经为负数
  Lon, eastern longitude is positive, west longitude is negative
getMaxMessageLength() - Method in class com.hsm.barcode.Decoder
  Retrieves the maximum message length capable of the Decoder.
getMaxValue() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取最大值，仅对值文件类型有效
  acquire maximum value, it is valid for value file type only
getMessage(int) - Method in class com.rscja.deviceapi.CardWithBYL
  将错误代码转换为语义消息
getMinValue() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取最小值，仅对值文件类型有效
  acquire minimum value, it is valid for value file type only
getMode() - Method in class com.rscja.deviceapi.RFIDWithUHF
  获取寻标签模式，仅R2000模块有效
  acquire tag searching mode, it is valid for R2000 only
getModel() - Static method in class com.rscja.deviceapi.DeviceConfiguration
  获取设备型号
  Acquire device model NO.
getMorphoDescriptor() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
getMorphoPIDSN() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  获取指纹版本
  acquire fingerprint version
getMorphoSecurityLevel() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
getNationalID() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的NationalID信息
  acquire national infor of animal tag
getNavType() - Method in class com.rscja.deviceapi.entity.BDLocation
getNumber() - Method in class com.rscja.deviceapi.entity.SatelliteEntity
getNumParameter(int) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  获取扫描头参数(此函数目前只支持moto扫描头)
  Acquire scanning module parameter(this formula supports MOTO scanning module only)
getNumProperty(int) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  获取扫描头属性(此函数目前只支持moto扫描头)
  acquire scanning module property(this formula supports MOTO scanning module only)
getOCRMode() - Method in class com.hsm.barcode.Decoder
  Gets the OCR Mode
getOCRTemplates() - Method in class com.hsm.barcode.Decoder
  Gets the OCR active template configuration.
getOCRUserTemplate() - Method in class com.hsm.barcode.Decoder
  Gets the OCR User defined template.
getOriginalUID() - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  获取标签原始的UID
  acquire original UID of tag
getPara(int) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  获取参数设置
getParam(char, char[]) - Method in class com.rscja.deviceapi.RFIDWithUHF
  获取模块参数，仅R2000模块有效
  acquire module parameter, it is valid for R2000 only
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHF
  读取模块的功率
  read power of module
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  读取模块的功率
getPreviewFrame(Bitmap) - Method in class com.hsm.barcode.Decoder
  Gets a single frame (1/4 size) from the engine.
getPsamCardID() - Method in class com.rscja.deviceapi.CardWithBYL
  获取psam卡id
getPSOCMajorRev() - Method in class com.hsm.barcode.Decoder
  Retrieves the Major revision of the PSOC of the connected Engine.
getPSOCMinorRev() - Method in class com.hsm.barcode.Decoder
  Retrieves the Minor revision of the PSOC of the connected Engine.
getPTInfo() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取模块信息
  Acquire module information
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHF
  获取占空比，仅适用于R2000模块
  acquire duty ratio, used for R2000 module only
getQTPara() - Method in class com.rscja.deviceapi.RFIDWithUHF
  获取是否开启寻隐藏区(仅R2000 QT标签)
  acquire hidden area activation or not (R2000 QT tag only)
getR2000Version() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  获取UHF R2000版本号
getRandomData() - Method in class com.rscja.deviceapi.Fingerprint
  获取随机数，检测模块是否正常
  Acquire random number, detect module is normal or not.
getRawData() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取原始数据，十六进制表示
  acquire original data, hexdecimal
getReadMode() - Method in class com.rscja.deviceapi.RFIDWithUHF
  获取读取模式
  acquire reading mode.
getReadPermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取读取权限
  acquire read authorization
getReadWritePermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取读写权限
  acquire read-write authorization
getReserved() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的Reserved信息
  acquire Reserved infor of animal tag
getResultData() - Method in class com.rscja.deviceapi.BDNavigation
  获取模块返回的原始数据
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHF
  获取链路参数，仅R2000有效
  acquire link parameter, R2000 is valid only.
getRTC() - Method in class com.rscja.deviceapi.RFIDWithUHF706
  获取RTC时间
getScanDriverRevision() - Method in class com.hsm.barcode.Decoder
  Retrieves the revision of the Scan Driver.
getScannerIdFromCamera(Context) - Static method in class com.zebra.adc.decoder.Barcode2DWithSoft
  此函数目前只支持moto 扫描头
  This formula supports MOTO scanning module only.
getScannerIdFromCamera2(Context) - Static method in class com.zebra.adc.decoder.Barcode2DWithSoft
  此函数目前只支持moto 扫描头
  This formula supports MOTO scanning module only.
getSecondaryDecoderRevision() - Method in class com.hsm.barcode.Decoder
  Deprecated.
  Secondary Decoder currently unsupported
getService() - Method in class com.rscja.deviceapi.service.BTService.LocalBinder
getShowDecodeWindow() - Method in class com.hsm.barcode.Decoder
  Retrieves the current show decode window setting.
getSignal() - Method in class com.rscja.deviceapi.entity.SatelliteEntity
getSingleFrame(Bitmap) - Method in class com.hsm.barcode.Decoder
  Gets a single frame from the engine.
getStatus(RFIDWithUHFBluetooth.StatusEnum, BluetoothDevice) - Method in interface com.rscja.deviceapi.RFIDWithUHFBluetooth.BTStatusCallback
getStatusMsg(int) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
getSTM32Version() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  获取UHF STM32版本号
getStrParameter(int) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  获取扫描头参数(此函数目前只支持moto扫描头)
  acquire scanning module parameter(this formula supports MOTO scanning module only)
getStrProperty(int) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  获取扫描头属性(此函数目前只支持moto扫描头)
  acquire scanning module property(this formula supports MOTO scanning module only)
getSupportedGattServices() - Method in class com.rscja.deviceapi.service.BTService
getSymbologyConfig(SymbologyConfig) - Method in class com.hsm.barcode.Decoder
  Retrieves the current configuration of the passed in structure.
getSymbologyConfigDefaults(SymbologyConfig) - Method in class com.hsm.barcode.Decoder
  Retrieves the default configuration of the passed in structure.
getSymbologyMaxRange(int) - Method in class com.hsm.barcode.Decoder
  Retrieves the maximum range of the passed in symbology ID.
getSymbologyMinRange(int) - Method in class com.hsm.barcode.Decoder
  Retrieves the minimum range of the passed in symbology ID.
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHF
  获取模块温度，模块在工作中不能获取文档。（仅R2000模块有效）
  acquire module temperature, module cannot acquire files in operation
getTimeToFirstFix() - Method in class com.rscja.deviceapi.BDNavigation
  获取第一次定位成功所用时间
  Acquire duration of first successful positioning.
getType() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签类型
  acquire tag type
getUart() - Method in class com.rscja.deviceapi.DeviceConfiguration
  获取串口路径
  Acquire serial port directory
getUID() - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  获取卡片ID
  Acquire card ID
getUIDBytes() - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  获取卡片ID
  Acquire card ID
getUIDWith4450Card() - Method in class com.rscja.deviceapi.RFIDWithLF
  获取UID,用于4450Card
  Acquire UID, used for 4450 card
getUIDWithHID() - Method in class com.rscja.deviceapi.RFIDWithLF
  读取HID卡
  Read HID card
getUIDWithHitagS() - Method in class com.rscja.deviceapi.RFIDWithLF
  获取UID,用于hitag S
  Acquire UID, used for hitag S
getUpdatePermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取修改权限
  acquire modify authorization
getValue() - Method in enum com.barcode.BarcodeUtility.ModuleType
getValue() - Method in enum com.rscja.deviceapi.Fingerprint.BufferEnum
  获取枚举的值
  Acquire example value
getValue() - Method in enum com.rscja.deviceapi.RFIDWithISO14443A.DESFireEncryptionTypekEnum
getValue() - Method in enum com.rscja.deviceapi.RFIDWithISO14443A.DESFireFileTypekEnum
getValue() - Method in enum com.rscja.deviceapi.RFIDWithISO15693.TagType
getValue() - Method in enum com.rscja.deviceapi.RFIDWithUHF.BankEnum
getValue() - Method in enum com.rscja.deviceapi.RFIDWithUHF.LockModeEnum
  Deprecated.
  获取枚举的值
  Acquire example value
getValue() - Method in enum com.rscja.deviceapi.RFIDWithUHF.SingleModeEnum
getValue() - Method in enum com.rscja.deviceapi.RFIDWithUHFBluetooth.BankEnum
getValue() - Method in enum com.zebra.adc.decoder.Barcode2DWithSoft.CODETYPE
getVersion() - Method in class com.rscja.deviceapi.Fingerprint
  获取模块版本
  Acquire module version
getVersion() - Static method in class com.rscja.deviceapi.VersionInfo
  获取jar包版本信息
  acquire jar pack version infor
getVersions() - Method in class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
  获取指纹模块版本号
  Acquire fingerprint module version
getWritePermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取写权限
  acquire write authorization
grab() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  采集图像
  Acquire image

A B C D E F G H I K L M N O P R S T U V W X Y