U-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## U

uartSwitch2(int) - Method in class com.rscja.deviceapi.Module
  Deprecated.
UHFBlockPermalock(String, int, int, int, String, int, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
uhfDeactivate(String, String, RFIDWithUHF.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  客户定制
  Customizing
uhfDecryptSM4(String, StringBuilder) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  数据解密
uhfDwell(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  * 客户定制
  Customizing
uhfEncReadUser(int, int, StringBuilder) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  user区数据解密
uhfEncryptSM4(String, StringBuilder) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  数据加密
uhfEncWriteUser(int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  user区加密
uhfEndUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  uhf模块升级结束
uhfGetSMKey(byte[], StringBuilder, StringBuilder) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  获取密码
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHF
  升级uhf模块
uhfReBoot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  uhf模块升级之前reboot
uhfSetSM4Key(int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  设置密码
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHF
  升级uhf模块
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  uhf模块升级开始
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHF
  升级uhf模块
UHFTAGInfo - Class in com.rscja.deviceapi.entity
UHFTAGInfo() - Constructor for class com.rscja.deviceapi.entity.UHFTAGInfo
uhfUpdateData(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  uhf模块升级中
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHF
  升级uhf模块
UNIFORM - Static variable in class com.hsm.barcode.ExposureValues.ExposureMethod
  Deprecated.
  Auto exposure is determined across entire image
UNKNOWN - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineID
  Unknown Engine ID
UNKNOWN - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineType
  Unknown Engine Type
upChar(Fingerprint.BufferEnum) - Method in class com.rscja.deviceapi.Fingerprint
  上传指定缓冲区中的指纹特征数据
  Upload fingerprint feature data of specified buffer zone
Upgrade(int, int, int, byte[]) - Method in class com.rscja.deviceapi.PSAM
  固件升级
  Firmware upgrade
upImage(int, String) - Method in class com.rscja.deviceapi.Fingerprint
  上传指纹图像文件
  Upload finerprint image file
UpperLeft_X_Max - Variable in class com.hsm.barcode.DecodeWindowing.DecodeWindowLimits
  Upper left X coordinate maximum value
UpperLeft_X_Min - Variable in class com.hsm.barcode.DecodeWindowing.DecodeWindowLimits
  Upper left X coordinate minimum value
UpperLeft_Y_Max - Variable in class com.hsm.barcode.DecodeWindowing.DecodeWindowLimits
  Upper left Y coordinate maximum value
UpperLeft_Y_Min - Variable in class com.hsm.barcode.DecodeWindowing.DecodeWindowLimits
  Upper left Y coordinate minimum value
UpperLeftX - Variable in class com.hsm.barcode.DecodeWindowing.DecodeWindow
  Upper left X coordinate setting
UpperLeftY - Variable in class com.hsm.barcode.DecodeWindowing.DecodeWindow
  Upper left Y coordinate setting
USER - Static variable in class com.hsm.barcode.DecoderConfigValues.OCRTemplate
  OCR User Template

A B C D E F G H I K L M N O P R S T U V W X Y