R-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## R

rats() - Method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  CPU卡RATS操作指令
  CPU card RATS operation command
RAW_BINARY - Static variable in class com.hsm.barcode.IQImagingProperties.IQImageFormat
  Raw Binary Image Format
RAW_GRAY - Static variable in class com.hsm.barcode.IQImagingProperties.IQImageFormat
  Raw Gray Image Format
read(String, RFIDWithISO14443A.KeyType, int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读卡,此函数包含寻卡和验证密钥步骤
  Read card, this formula includes card search and key verfication procedure
read(int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读卡，适用于Urltra light标签
  card reading, used for Urltra light tag
read(int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  读取块数据
  read block data
read(int, int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  读取块数据
  block data
readAllData(String, RFIDWithISO14443A.TagType) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读卡，读取卡片所有块中的数据
  Card reading, read data of all blocks in the card
readAnimalTags(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读取动物标签信息
  read animal tag infor
readCameraState() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  读取camera状态
  read camera status
readCharacteristic(BluetoothGattCharacteristic) - Method in class com.rscja.deviceapi.service.BTService
readChipSN() - Method in class com.rscja.deviceapi.Fingerprint
  获取芯片序列号
  acquire chip serial number
readData(String, RFIDWithUHF.BankEnum, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  读取标签某个存储区的所有数据（指定UII）。芯联模块不支持
  Read all the data of random storage of tags (specified UII).
readData(String, RFIDWithUHF.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
readData(String, RFIDWithUHF.BankEnum, int, int, String, RFIDWithUHF.BankEnum, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  读取标签某个存储区的所有数据
  Read all the data of random storage of tags
readData(String, RFIDWithUHFBluetooth.BankEnum, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  读取标签数据
readData(String, RFIDWithUHFBluetooth.BankEnum, int, int, String, RFIDWithUHFBluetooth.BankEnum, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  读取标签数据
readDataWith4305Card(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读4305卡的某一页（0~31）数据
  read card 4305 data of random page (0-31)
readDataWithHitagS(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读取Hitag S卡中的某一页的数据
  Read data of random page in Hitag S card
readDataWithIDCard(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读卡,用于ID卡
  card reading, used for ID card
readDataWithQT(String, RFIDWithUHF.BankEnum, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  读取标签数据（不指定UII）,用于R2000 QT标签
  read tag data ( non-specified UII), used for R2000 QT tag
readDataWithQT(String, RFIDWithUHF.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
readDataWithQT(String, RFIDWithUHF.BankEnum, int, int, String, RFIDWithUHF.BankEnum, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  读取标签某个存储区的所有数据,用于R2000 QT标签
  read all data of random storage of the tag, used for R2000 QT tag.
readInfo() - Method in class com.rscja.deviceapi.RFIDWithUHF706
  安全模块主动向设备上传识读信息
readScannerCameraId() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  读取camera id
  read camera id
readSysPara() - Method in class com.rscja.deviceapi.Fingerprint
  获取系统参数，仅返回版本号
  Acquire system parameter, return version number only
readSysParaMore() - Method in class com.rscja.deviceapi.Fingerprint
  获取系统参数
  Acquire system parameter
readTagData_sf() - Method in class com.rscja.deviceapi.RFIDWithUHF
  顺丰定制接口
  Customizing
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHF
  读取缓冲区返回的标签的TID和UII
  read return TID and UII infor of tag in buffer zone.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  读取标签数据
readTagFromR2000Buffer() - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
readUidFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHF
  读取缓冲区返回的标签UII
  read the return tag UII in buffer zone
readUnsignedInt64(byte[]) - Static method in class com.rscja.utility.StringUtility
  读取无符号位的长整数，64位
readWithNeedleTag() - Method in class com.rscja.deviceapi.RFIDWithLF
  读数据，针对针管标签
  read data, for needle tube tag
receive() - Method in class com.rscja.deviceapi.Infrared
  接收数据
  Receive data
receive() - Method in class com.rscja.deviceapi.Module
  接收数据
  Receive data
receiveData(byte[]) - Method in class com.rscja.deviceapi.Printer
  接收串口数据
  receive serial port data
receiveData() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  (备注:禁止使用)
receiveData(byte[], boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  (备注:禁止使用)
receiveDataTAG() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  (备注:禁止使用)
regModel() - Method in class com.rscja.deviceapi.Fingerprint
  合并特征文件。将模板缓冲区1与模板缓冲区2中的模板文件合并生成模板，结果存于模板缓冲区1。
  Combine feature file.
request() - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  寻卡
  Search card
requestRandom() - Method in class com.rscja.deviceapi.RFIDWithUHF706
  向安全模块请求随机数
requsetReadPart(byte, byte, byte, byte, byte, byte) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  读分区请求
requsetWritePart(byte[], byte, byte, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  写分区请求
Reserved - Variable in class com.hsm.barcode.IQImagingProperties
  Must be set to -1
reset() - Method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  CPU卡复位操作指令
  CPU card reset operation command
reset() - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  CPU卡复位操作指令
  CPU card reset operation commande
Resolution - Variable in class com.hsm.barcode.IQImagingProperties
  # pixels/IntellBarcodeUnits (Practical range 1 to 100)
responseCancel() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  取消当前操作
  Cancel current operation
responseContinue() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  继续当前操作
  Continue current operation
restoreDefault() - Method in class com.rscja.deviceapi.Printer
  参数还原默认值
  parameter reset to default
RESULT_ERR_BADREGION - Static variable in class com.hsm.barcode.DecoderException.ResultID
  An image was requested using an invalid image region
RESULT_ERR_BADSMARTIMAGE - Static variable in class com.hsm.barcode.DecoderException.ResultID
  IQ image fail
RESULT_ERR_CANCEL - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Asynchronous decode was canceled
RESULT_ERR_DRIVER - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Error detected in image engine driver
RESULT_ERR_ENGINEBUSY - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Image engine driver reported busy
RESULT_ERR_EXCEPTION - Static variable in class com.hsm.barcode.DecoderException.ResultID
  An exception was detected in the deoder
RESULT_ERR_EXMFILE_INVALID - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Not a valid configuration file.
RESULT_ERR_LOAD_EXMFILE - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Error loading EXM file.
RESULT_ERR_MEMORY - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Memory allocation failed
RESULT_ERR_MISSING_EXMSECTION - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Section missing from exm file.
RESULT_ERR_NODATA - Static variable in class com.hsm.barcode.DecoderException.ResultID
  No data to send
RESULT_ERR_NODECODE - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Image engine unable to decode a symbology
RESULT_ERR_NOIMAGE - Static variable in class com.hsm.barcode.DecoderException.ResultID
  No image available
RESULT_ERR_NORESPONSE - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Could not communicate with imager
RESULT_ERR_NOTCONNECTED - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Not connected to image engine
RESULT_ERR_NOTRIGGER - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Trigger state is false
RESULT_ERR_PARAMETER - Static variable in class com.hsm.barcode.DecoderException.ResultID
  One of the function parameters was invalid
RESULT_ERR_PROCESSING_EXMSECTION - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Error processing exm file section.
RESULT_ERR_SMARTIMAGETOOLARGE - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Requested IQ image too large
RESULT_ERR_THREAD - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Could not create async decode thread
RESULT_ERR_TOO_MUCH_INTERPOLATION - Static variable in class com.hsm.barcode.DecoderException.ResultID
  IQ image fail
RESULT_ERR_UNSUPPORTED - Static variable in class com.hsm.barcode.DecoderException.ResultID
  The operation was not supported by the engine
RESULT_ERR_UNSUPPORTED_IQ_BARCODE - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Scanned barcode is not a valid IQ host barcode
RESULT_ERR_WRONGRESULTSTRUCT - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Invalid structure size
RESULT_INITIALIZE - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Initialize
RESULT_SUCCESS - Static variable in class com.hsm.barcode.DecoderException.ResultID
  Operation was successful
ResultALLRawData(String) - Method in interface com.rscja.deviceapi.BDNavigation.TestResultRawData
  返回String类型
  Returned String type
ResultALLRawData(byte[], int) - Method in interface com.rscja.deviceapi.BDNavigation.TestResultRawData
  返回byte[]
  Returned byte[]
reverse(byte[]) - Static method in class com.rscja.utility.StringUtility
  逆转字节数组
RFIDArgumentException - Exception in com.rscja.deviceapi.exception
  参数错误异常
  parameter err
RFIDArgumentException(String) - Constructor for exception com.rscja.deviceapi.exception.RFIDArgumentException
RFIDNotFoundException - Exception in com.rscja.deviceapi.exception
  寻卡失败异常
  card searching failed err
RFIDNotFoundException() - Constructor for exception com.rscja.deviceapi.exception.RFIDNotFoundException
RFIDReadFailureException - Exception in com.rscja.deviceapi.exception
  读卡失败异常
  card reading failure err
RFIDReadFailureException() - Constructor for exception com.rscja.deviceapi.exception.RFIDReadFailureException
RFIDVerificationException - Exception in com.rscja.deviceapi.exception
  验证失败异常
  verify failure err
RFIDVerificationException() - Constructor for exception com.rscja.deviceapi.exception.RFIDVerificationException
RFIDWithISO14443A - Class in com.rscja.deviceapi
  RFID模块ISO14443A协议操作类
  RFID module ISO 14443A protocol operation type
RFIDWithISO14443A.DESFireEncryptionTypekEnum - Enum in com.rscja.deviceapi
  DESFire卡加密类型
  DESFire card encyption type
RFIDWithISO14443A.DESFireFileTypekEnum - Enum in com.rscja.deviceapi
  DESFire卡文件类型
  DESFire card file typr
RFIDWithISO14443A.KeyType - Enum in com.rscja.deviceapi
  密钥类型，适用于S50和S70标签。
  key type, used for S50 and S70 tags.
RFIDWithISO14443A.TagType - Enum in com.rscja.deviceapi
  M1标签类型定义
  M1 tag type definition
RFIDWithISO14443A4CPU - Class in com.rscja.deviceapi
  RFID模块ISO14443A CPU卡协议操作类
  RFID module ISO14443A CPU card protocol operation type
RFIDWithISO14443B - Class in com.rscja.deviceapi
  RFID模块ISO14443B协议操作类
  RFID module ISO14443B protocol operation type
RFIDWithISO15693 - Class in com.rscja.deviceapi
  RFID模块ISO15693协议操作类,
  RFID module ISO15639 protocol operation type
RFIDWithISO15693.TagType - Enum in com.rscja.deviceapi
  标签类型
  Tag type
RFIDWithLF - Class in com.rscja.deviceapi
  RFID低频（125K）操作类
  RFID LF (125K) operation type
RFIDWithUHF - Class in com.rscja.deviceapi
  UHF模块操作类
  UHF module operation type
RFIDWithUHF.BankEnum - Enum in com.rscja.deviceapi
  存储区
  Storage
RFIDWithUHF.LockModeEnum - Enum in com.rscja.deviceapi
  Deprecated.
RFIDWithUHF.SingleModeEnum - Enum in com.rscja.deviceapi
  读取模式
  Read mode
RFIDWithUHF706 - Class in com.rscja.deviceapi
  UHF 706所模块操作类
RFIDWithUHFBluetooth - Class in com.rscja.deviceapi
RFIDWithUHFBluetooth.BankEnum - Enum in com.rscja.deviceapi
  存储区
  Storage
RFIDWithUHFBluetooth.BTStatusCallback - Interface in com.rscja.deviceapi
  连接蓝牙的状态值回调
RFIDWithUHFBluetooth.KeyEventCallback - Interface in com.rscja.deviceapi
  接收扫描按键的回调
RFIDWithUHFBluetooth.ScanBTCallback - Interface in com.rscja.deviceapi
  扫描蓝牙设备的回调接口
RFIDWithUHFBluetooth.StatusEnum - Enum in com.rscja.deviceapi
  蓝牙状态枚举 CONNECTED:已经连接
  DISCONNECTED:已经断开
  CONNECTING:连接中
rIndex - Static variable in class com.rscja.deviceapi.RFIDWithUHFBluetooth
rIndexTAG - Static variable in class com.rscja.deviceapi.RFIDWithUHFBluetooth
Rotation - Variable in class com.hsm.barcode.ImagerProperties
  Image rotation value
Rows - Variable in class com.hsm.barcode.ImagerProperties
  Height of image
RX_CHAR_UUID - Static variable in class com.rscja.deviceapi.service.BTService
RX_SERVICE_UUID - Static variable in class com.rscja.deviceapi.service.BTService

A B C D E F G H I K L M N O P R S T U V W X Y