C-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## C

C4000_6577 - Static variable in class com.rscja.deviceapi.DeviceConfiguration
C4000_6582 - Static variable in class com.rscja.deviceapi.DeviceConfiguration
C4050_6582 - Static variable in class com.rscja.deviceapi.DeviceConfiguration
C4050_8909 - Static variable in class com.rscja.deviceapi.DeviceConfiguration
C6000_6735 - Static variable in class com.rscja.deviceapi.DeviceConfiguration
C6000_8909 - Static variable in class com.rscja.deviceapi.DeviceConfiguration
C70_6735 - Static variable in class com.rscja.deviceapi.DeviceConfiguration
C72_6735 - Static variable in class com.rscja.deviceapi.DeviceConfiguration
C76_6735 - Static variable in class com.rscja.deviceapi.DeviceConfiguration
callbackKeepGoing() - Method in class com.hsm.barcode.Decoder
  Callback used to stop decoding.
callbackMultiRead() - Method in class com.hsm.barcode.Decoder
  Callback used for MultiRead (Shotgun).
CallbackWaitTimeout - Variable in class com.hsm.barcode.DecodeOptions
  Deprecated.
  Timeout setting decWaitForDecode will wait before checking callback (WinCE Only)
cardConsumeConfirm(String, String, String) - Method in class com.rscja.deviceapi.CardWithBYL
CardWithBYL - Class in com.rscja.deviceapi
  白玉兰公交卡操作类
CCCD - Static variable in class com.rscja.deviceapi.service.BTService
CENTER_ONLY - Static variable in class com.hsm.barcode.ExposureValues.ExposureMethod
  Deprecated.
  Auto exposure is determined based on center only
CENTER_WEIGHTED - Static variable in class com.hsm.barcode.ExposureValues.ExposureMethod
  Deprecated.
  Auto exposure is determined based primarily on center only, but weighted
changeBDProvider(BDNavigation.BDProviderEnum) - Method in class com.rscja.deviceapi.BDNavigation
  改变参与定位的卫星系统
  Change positioning satellite system
changeBDStartMode(BDNavigation.BDStartModeEnum) - Method in class com.rscja.deviceapi.BDNavigation
  模块改变启动模式
  Module change start mode
char2HexString(char) - Static method in class com.rscja.utility.StringUtility
  char转十六进制
charArrayTolong(char[]) - Static method in class com.rscja.utility.StringUtility
  将8字节的Char数组转成一个long值
chars2HexString(char[], int) - Static method in class com.rscja.utility.StringUtility
  char类型数组转十六进制字符串
chars2Long(char[], int, int) - Static method in class com.rscja.utility.StringUtility
  char数组转long
charsTobytes(char[], int) - Static method in class com.rscja.utility.StringUtility
cleanFaultCard() - Method in class com.rscja.deviceapi.CardWithBYL
  清除故障卡
clearCache() - Method in class com.rscja.deviceapi.Printer
  立即清空打印缓存,清空打印机接收缓冲区和打印缓冲区
  Clear up printing cache, clear printer receive zone and buffer zone
close(Context, BarcodeUtility.ModuleType) - Method in class com.barcode.BarcodeUtility
  关闭指定功能 Switch off designated function
close() - Method in class com.rscja.deviceapi.Barcode1D
  关闭一维扫描设备
  Switch off 1D barcode scanning device.
close() - Method in class com.rscja.deviceapi.Barcode2D
  关闭二维扫描设备
  Switch off 2D barcode scanning device.
close() - Method in class com.rscja.deviceapi.BDNavigation
  关闭北斗导航模块
  Switch off Beidou navigation module.
close() - Method in class com.rscja.deviceapi.Infrared
  关闭红外模块
  Switch off infared module
close() - Method in class com.rscja.deviceapi.LedLight
  关闭LED灯
  Switch off LED
close() - Method in class com.rscja.deviceapi.service.BTService
close() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  关闭二维扫描设备
  Switch off 2D barcode scannning device
closeAuxiliaryLight(Context) - Method in class com.rscja.deviceapi.ScanerLedLight
  关闭扫描辅助灯，目前只支持C70系列
  Switch on scanning light, support C70 series only
closeKeyboardHelper(Context) - Method in class com.barcode.BarcodeUtility
  关闭键盘助手功能总开关 Switch off main function switch of keyboardemulator
closeLED() - Method in class com.rscja.deviceapi.Infrared
  关闭辅助灯
  Close LED
codeId - Variable in class com.hsm.barcode.DecodeResult
  This variable will contain the Honeywell Code ID for the decoded symbology
ColorFormat - Variable in class com.hsm.barcode.ImagerProperties
  Color format of image
Columns - Variable in class com.hsm.barcode.ImagerProperties
  Width of image
com.barcode - package com.barcode
com.hsm.barcode - package com.hsm.barcode
com.rscja.deviceapi - package com.rscja.deviceapi
com.rscja.deviceapi.entity - package com.rscja.deviceapi.entity
com.rscja.deviceapi.exception - package com.rscja.deviceapi.exception
com.rscja.deviceapi.service - package com.rscja.deviceapi.service
com.rscja.utility - package com.rscja.utility
com.zebra.adc.decoder - package com.zebra.adc.decoder
CONCURRENT - Static variable in class com.hsm.barcode.DecoderConfigValues.LightsMode
  Both aimer and illumination
configFDXTag(char[], char[]) - Method in class com.rscja.deviceapi.RFIDWithLF
  EM4305 配置成动物标签
  EM4305 configurate animal tag
ConfigurationException - Exception in com.rscja.deviceapi.exception
  设备配置异常类
  Device configuration exception type
ConfigurationException() - Constructor for exception com.rscja.deviceapi.exception.ConfigurationException
CONFORM_IMAGE - Static variable in class com.hsm.barcode.ExposureValues.ConformImage
  Image must conform to exposure settings
ConformImage() - Constructor for class com.hsm.barcode.ExposureValues.ConformImage
connect(String, RFIDWithUHFBluetooth.BTStatusCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  连接蓝牙设备
connect(String, RFIDWithUHFBluetooth.BTStatusCallback) - Method in class com.rscja.deviceapi.service.BTService
connectDecoderLibrary() - Method in class com.hsm.barcode.Decoder
  Method used to connect to the engine and initialize the API.
Consume(float) - Method in class com.rscja.deviceapi.CardWithBYL
  扣费
convertUiiToEPC(String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  UII转EPC
  UII transform to EPC
crcOff() - Method in class com.rscja.deviceapi.RFIDWithUHF
  取消CRC校验
crcOn() - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置CRC校验
  setup CRC verification

A B C D E F G H I K L M N O P R S T U V W X Y