I-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## I

ILLUM_AIM_OFF - Static variable in class com.hsm.barcode.DecoderConfigValues.LightsMode
  Neither aimer or illumination
ILLUM_AIM_ON - Static variable in class com.hsm.barcode.DecoderConfigValues.LightsMode
  Aimer and illumination alternating
ILLUM_ONLY - Static variable in class com.hsm.barcode.DecoderConfigValues.LightsMode
  Illumination only
IllumColor - Variable in class com.hsm.barcode.ImagerProperties
  Color of illumination
IlluminationClipValue - Variable in class com.hsm.barcode.ImageAttributes
  Deprecated.
  Illumination clip value
IlluminationMaxValue - Variable in class com.hsm.barcode.ImageAttributes
  Illumination white value max
IlluminationValue - Variable in class com.hsm.barcode.ImageAttributes
  Illumination white value
ImageAttributes - Class in com.hsm.barcode
  Image Attributes class defining image information
ImageAttributes() - Constructor for class com.hsm.barcode.ImageAttributes
  Data structure that is used to retrieve attributes of last acquired image
IMAGER - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineType
  Imager Engine Type
IMAGER_4200_ENGINE - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineID
  Deprecated.
  4200 Engine ID
IMAGER_IT4000_ENGINE - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineID
  Deprecated.
  IT4000 Engine ID
IMAGER_IT4100_ENGINE - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineID
  Deprecated.
  IT4100 Engine ID
IMAGER_IT4300_ENGINE - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineID
  Deprecated.
  IT4300 Engine ID
IMAGER_IT5100_ENGINE - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineID
  IT5100 Engine ID
IMAGER_IT5300_ENGINE - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineID
  IT5300 Engine ID
IMAGER_N5600_ENGINE - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineID
  N5600 Engine ID
IMAGER_N5603_ENGINE - Static variable in class com.hsm.barcode.DecoderConfigValues.EngineID
  N5603 Engine ID
ImagerProperties - Class in com.hsm.barcode
  Imager properties of connected engine.
ImagerProperties() - Constructor for class com.hsm.barcode.ImagerProperties
  Imager Properties structure containing information about connected engine
ImageSize - Variable in class com.hsm.barcode.ImageAttributes
  Size of the image
Infrared - Class in com.rscja.deviceapi
  红外模块操作类 Infared module operation type
init() - Method in class com.rscja.deviceapi.CardWithBYL
  初始化RFID和PSAM模块
init() - Method in class com.rscja.deviceapi.Fingerprint
  初始化指纹模块，默认波特率为57600
  Initialize fingerprint module, default baud rate is 57600.
init(int) - Method in class com.rscja.deviceapi.Fingerprint
  初始化指纹模块
  Initialize fingerprint module.
init(Context) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  初始化指纹模块
  Initialize fingerprint module
init() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  初始化指纹模块
  Initialize fingerprint module
init() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  初始化指纹模块
  Initialize fingerprint module
init(int) - Method in class com.rscja.deviceapi.Module
  初始化模块
  Initialize module
init(int, int) - Method in class com.rscja.deviceapi.Module
  初始化模块
init() - Method in class com.rscja.deviceapi.Printer
  打开打印机模块
  Switch on printer module
init() - Method in class com.rscja.deviceapi.PSAM
  初始化PSAM
  Initialize PSAM
init() - Method in class com.rscja.deviceapi.RFIDWithLF
  初始化RFID低频模块
  Initialize RFID LF module
init() - Method in class com.rscja.deviceapi.RFIDWithUHF
  初始化UHF模块,适应所有模块
  Initialize UHF module(Support all modules)
init() - Method in class com.rscja.deviceapi.RFIDWithUHF706
  初始化UHF模块
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  初始化蓝牙服务
init() - Method in class com.rscja.deviceapi.ScanerLedLight
  初始化设备资源
  initialize device source
init_R2000() - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
initialize() - Method in class com.rscja.deviceapi.service.BTService
initWithNeedleTag() - Method in class com.rscja.deviceapi.RFIDWithLF
  初始化RFID低频模块，针对针管标签
  Initialize RFID LF module, for needle tube tag
int2Bytes(int) - Static method in class com.rscja.utility.StringUtility
  int转byte数组
Int2bytes(int) - Static method in class com.rscja.utility.StringUtility
int2HexString(int) - Static method in class com.rscja.utility.StringUtility
interceptTrimLeft(Context, int) - Method in class com.barcode.BarcodeUtility
  截取左边字符串数量 Capture left side charactor string amount
interceptTrimRight(Context, int) - Method in class com.barcode.BarcodeUtility
  截取右边字符串数量 Capture right side charactor string amount
ints2HexString(int[], int) - Static method in class com.rscja.utility.StringUtility
inventory() - Method in class com.rscja.deviceapi.RFIDWithISO15693
  读卡
  read card
inventoryBank_sf(String, char, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  顺丰定制接口
  Customizing
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHF
  该函数单步识别标签，一次只返回一个UII
  this formula identify tag in single step, return UII for only one time.
inventorySingleTag_sf() - Method in class com.rscja.deviceapi.RFIDWithUHF
  顺丰定制接口
  Customizing
inventorySingleTag_tc(int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  客户定制函数/Customizing 该函数单步识别标签，一次只返回一个UII
  this formula identify tag in single step, return UII for only one time.
inventorySingleTagBytes() - Method in class com.rscja.deviceapi.RFIDWithUHF
  该函数单步识别标签，一次只返回一个UII
  this formula will identify tag in single step, return one UII for one time
inventorySingleTagWithR2000() - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
ioctl_gpio(int, boolean) - Method in class com.rscja.deviceapi.Module
IQImagingProperties - Class in com.hsm.barcode
  IQ Imaging Class
IQImagingProperties() - Constructor for class com.hsm.barcode.IQImagingProperties
  Class for IQ Imaging Structure that defines the parameters used during the attempt to acquire an Intelligent Image
IQImagingProperties.IQImageFormat - Class in com.hsm.barcode
  Defines the supported image formats for Intelligent Imaging
ISBN - Static variable in class com.hsm.barcode.DecoderConfigValues.OCRTemplate
  OCR ISBN Template
isDecimal(String) - Static method in class com.rscja.utility.StringUtility
  判断字符串是否是十进制数字
isEmpty(CharSequence) - Static method in class com.rscja.utility.StringUtility
  判断字符串是否为空
isHexNumber(String) - Static method in class com.rscja.utility.StringUtility
  Deprecated.
isHexNumberRex(String) - Static method in class com.rscja.utility.StringUtility
  判断字符串是否是十六进制数字，使用正则表达式方式
isNum(String) - Static method in class com.rscja.utility.StringUtility
  判断是否为数字
ISO14443A_decrement(int, int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
ISO14443A_increment(int, int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  电子钱包充值
  E-wallet charge
ISO14443A_initval(int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  电子钱包初始化
  E-wallet initialize
ISO14443A_readval(int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读取电子钱包余额 传入参数
  read E-wallet balance
ISO15693Entity - Class in com.rscja.deviceapi.entity
  ISO15693协议数据实体
  ISO15639 protocol data entity
ISO15693Entity(String, String) - Constructor for class com.rscja.deviceapi.entity.ISO15693Entity
  构造函数
  Constructor
ISO15693Entity(String, String, char[]) - Constructor for class com.rscja.deviceapi.entity.ISO15693Entity
  构造函数
  Constructor
ISO15693Entity(String, String, char[], byte[]) - Constructor for class com.rscja.deviceapi.entity.ISO15693Entity
ISO15693Entity(String, String, char[], String, String) - Constructor for class com.rscja.deviceapi.entity.ISO15693Entity
  构造函数
  Constructor
isOctNumber(String) - Static method in class com.rscja.utility.StringUtility
  判断字符串是否是十进制数字
isOctNumberRex(String) - Static method in class com.rscja.utility.StringUtility
  判断字符串是否是十进制数字，使用正则表达式方式
isPowerOn() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  判断设备是否上电
  Determine whether the device is powered on.
isStop - Static variable in class com.rscja.deviceapi.RFIDWithUHFBluetooth
isUpAndroid7() - Static method in class com.zebra.adc.decoder.Barcode2DWithSoft
isWrite - Static variable in class com.rscja.deviceapi.service.BTService

A B C D E F G H I K L M N O P R S T U V W X Y