E-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## E

EM125k_ReadHitag1() - Method in class com.rscja.deviceapi.RFIDWithLF
  获取所有页的数据
  Acquire data of all pages
empty() - Method in class com.rscja.deviceapi.Fingerprint
  清空模块中保存的指纹数据
  empty out saved fingerprint data in module.
enableAllCodeTypes() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  开启所有类型条码识别
  activate all types of barcodes identification
enableBarcode(SymbologyConfiguration.BarcodeSymbologyID, SymbologyConfig) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  开启条码(此函数目前只支持6603扫描头)
  activate barcode(this formula supports 6603 scanning module only)
enableContinuousScan(Context, boolean) - Method in class com.barcode.BarcodeUtility
  启用连续扫描 Enable continuous scan
enableEnter(Context, boolean) - Method in class com.barcode.BarcodeUtility
  是否启用回车 Whether enable Enter function
enablePlayFailureSound(Context, boolean) - Method in class com.barcode.BarcodeUtility
  扫描失败是否播放提示音 whether playing notification when scanning failure.
enablePlaySuccessSound(Context, boolean) - Method in class com.barcode.BarcodeUtility
  是否播放成功的提示音 whether playing notification when scanning success.
enableSymbology(int) - Method in class com.hsm.barcode.Decoder
  Enables the passed in symbology ID.
enableTAB(Context, boolean) - Method in class com.barcode.BarcodeUtility
  是否启用TAB Whether enable TAB function
enableTXNotification() - Method in class com.rscja.deviceapi.service.BTService
enableVibrate(Context, boolean) - Method in class com.barcode.BarcodeUtility
  扫描成功是否震动提示 whether vibrating when scanning success
Encryption(byte[], int) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  Deprecated.
Encryption(byte[], int, String) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  Deprecated.
EngineID - Variable in class com.hsm.barcode.ImagerProperties
  Engine ID of connected engine
EnginePartNum - Variable in class com.hsm.barcode.ImagerProperties
  Engine part number
EngineSerialNum - Variable in class com.hsm.barcode.ImagerProperties
  Engine serial number
enroll() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  采集指纹
  Acquire fingerprint
equals(Object) - Method in class com.rscja.deviceapi.entity.BDLocation
equals(Object) - Method in class com.rscja.deviceapi.entity.SatelliteEntity
eraseData(String, RFIDWithUHF.BankEnum, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  擦除标签数据（不指定UII）
  erase tag data ( non-specified UII)
eraseData(String, RFIDWithUHF.BankEnum, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  擦除标签数据（指定UII）
  erase tag data (specified UII)
eraseData(String, RFIDWithUHF.BankEnum, int, int, String, RFIDWithUHF.BankEnum, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
EventReport() - Method in class com.rscja.deviceapi.RFIDWithUHF706
  停止读
executeCmd(String, String) - Method in class com.rscja.deviceapi.PSAM
  执行PSAM命令
  Execute PSAM command
ExposureMethod() - Constructor for class com.hsm.barcode.ExposureValues.ExposureMethod
  Deprecated.
ExposureMode() - Constructor for class com.hsm.barcode.ExposureValues.ExposureMode
ExposureSettings() - Constructor for class com.hsm.barcode.ExposureValues.ExposureSettings
ExposureSettingsMinMax() - Constructor for class com.hsm.barcode.ExposureValues.ExposureSettingsMinMax
ExposureValue - Variable in class com.hsm.barcode.ImageAttributes
  Exposure valid settled on for the last image capture
ExposureValues - Class in com.hsm.barcode
ExposureValues.ConformImage - Class in com.hsm.barcode
  ConformImage class that defines whether or not the image should conform to exposure settings.
ExposureValues.ExposureMethod - Class in com.hsm.barcode
  Deprecated.
  ExposureMethod class that defines the auto exposure method that will be used during image capture.
ExposureValues.ExposureMode - Class in com.hsm.barcode
  ExposureMode class that defines the exposure mode that will be used during image capture.
ExposureValues.ExposureSettings - Class in com.hsm.barcode
  ExpsoureSettings class that defines most common setting used during image acquisition.
ExposureValues.ExposureSettingsMinMax - Class in com.hsm.barcode
  ExposureSettingsMinMax class that defines Minimum and Maximum settings for ExposureSettings
ExposureValues.SpecularExclusion - Class in com.hsm.barcode
  Deprecated.
  SpecularExclusion class that defines the specular exclusion setting in the ExposureSettings class that will be used during image capture.
EXTRA_DATA - Static variable in class com.rscja.deviceapi.service.BTService

A B C D E F G H I K L M N O P R S T U V W X Y