F-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## F

filterCharacter(Context, String) - Method in class com.barcode.BarcodeUtility
  过滤字符串 Filter charactor string
Fingerprint - Class in com.rscja.deviceapi
  指纹识别模块操作类,
  Fingerprint identify module operation type
Fingerprint.BufferEnum - Enum in com.rscja.deviceapi
  模块缓冲区枚举
  Module buffer zone example.
FingerprintAlreadyEnrolledException - Exception in com.rscja.deviceapi.exception
  指纹已经存在异常类
  fingerprint has exception type
FingerprintAlreadyEnrolledException() - Constructor for exception com.rscja.deviceapi.exception.FingerprintAlreadyEnrolledException
FingerprintInfo() - Constructor for class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
FingerprintInvalidIDException - Exception in com.rscja.deviceapi.exception
  ID已被占用异常类
  ID has been occupied exception type
FingerprintInvalidIDException() - Constructor for exception com.rscja.deviceapi.exception.FingerprintInvalidIDException
FingerprintWithFIPS - Class in com.rscja.deviceapi
  FIPS指纹识别模块操作类,
  FIPS fingerprint indentify module operation type,
FingerprintWithFIPS.DataFormat - Enum in com.rscja.deviceapi
  指纹数据格式
  Fingerprint data format
FingerprintWithFIPS.EnrollCallBack - Interface in com.rscja.deviceapi
  采集指纹回调接口
  call-back contact for acquiring fingerprint
FingerprintWithFIPS.FingerprintInfo - Class in com.rscja.deviceapi
FingerprintWithFIPS.GRABCallBack - Interface in com.rscja.deviceapi
  指纹图像回调接口
  fingerprint image call-back contact
FingerprintWithFIPS.IdentificationCallBack - Interface in com.rscja.deviceapi
  验证指纹的回调接口
  call-back contact of verify fingerprint
FingerprintWithFIPS.PtCaptureCallBack - Interface in com.rscja.deviceapi
  获取指纹模版数据回调接口
  Acquire call-back contact fingerprint template data
FingerprintWithFIPS.TemplateVerifyCallBack - Interface in com.rscja.deviceapi
  指纹模版比对
  fingerprint template comparison
FingerprintWithMorpho - Class in com.rscja.deviceapi
FingerprintWithMorpho.EnrollCallBack - Interface in com.rscja.deviceapi
  采集指纹回调接口
  acquire fingerprint call-back contact
FingerprintWithMorpho.IdentificationCallBack - Interface in com.rscja.deviceapi
  验证指纹的回调接口
  call-back contact for fingerprint verification
FingerprintWithMorpho.PtCaptureCallBack - Interface in com.rscja.deviceapi
  设置获取指纹模版回调接口
  setup fingerprint template acquire call-back contact
FingerprintWithMorpho.TemplateVerifyCallBack - Interface in com.rscja.deviceapi
FIRMWARE_REVISON_UUID - Static variable in class com.rscja.deviceapi.service.BTService
FirmwareEngineID - Variable in class com.hsm.barcode.ImagerProperties
  Engine Firmware ID
FIXED - Static variable in class com.hsm.barcode.ExposureValues.ExposureMode
  Fixed exposure
Flags - Variable in class com.hsm.barcode.SymbologyConfig
  Logical OR of valid flags for the given symbology
Format - Variable in class com.hsm.barcode.IQImagingProperties
  IQ Image Format
free() - Method in class com.rscja.deviceapi.CardWithBYL
  释放模块
free() - Method in class com.rscja.deviceapi.Fingerprint
  释放指纹模块
  Release fingerprint module.
free() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  释放指纹模块
  Release fingerprint module
free() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  释放指纹模块
  free fingerprint module
free() - Method in class com.rscja.deviceapi.Module
  释放模块
  Release module
free() - Method in class com.rscja.deviceapi.Printer
  关闭打印机模块
  Switch off printer module
free() - Method in class com.rscja.deviceapi.PSAM
  释放PSAM
  Release PSAM
free() - Method in class com.rscja.deviceapi.RFIDWithLF
  释放RFID低频模块
  Release RFID LF module
free() - Method in class com.rscja.deviceapi.RFIDWithUHF
  关闭UHF模块
  Switch off UHF module
free() - Method in class com.rscja.deviceapi.RFIDWithUHF706
  关闭UHF模块
free() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  释放已经占用的蓝牙服务资源
free() - Method in class com.rscja.deviceapi.ScanerLedLight
  释放设备资源
  release device source

A B C D E F G H I K L M N O P R S T U V W X Y