S-Index

A B C D E F G H I K L M N O P R S T U V W X Y

## S

SatelliteEntity - Class in com.rscja.deviceapi.entity
  卫星信息数据实体
  satellite infor data entity
SatelliteEntity(String, String) - Constructor for class com.rscja.deviceapi.entity.SatelliteEntity
scan() - Method in class com.rscja.deviceapi.Barcode1D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scan() - Method in class com.rscja.deviceapi.Barcode2D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scan() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  触发二维条码扫描
  Trigger 2D barcode scanning function
scanBarcode() - Method in class com.rscja.deviceapi.Barcode1D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBarcode() - Method in class com.rscja.deviceapi.Barcode2D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBTDevices(RFIDWithUHFBluetooth.ScanBTCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  扫描蓝牙设备
ScanerLedLight - Class in com.rscja.deviceapi
  扫描LED灯控制类（仅C6000有效）
  Scanning LED light control type ( valid for C6000 only)
ScanerLedLight() - Constructor for class com.rscja.deviceapi.ScanerLedLight
ScanerParamNum() - Constructor for class com.zebra.adc.decoder.Barcode2DWithSoft.ScanerParamNum
ScanerParamVal() - Constructor for class com.zebra.adc.decoder.Barcode2DWithSoft.ScanerParamVal
ScanerPropertyNum() - Constructor for class com.zebra.adc.decoder.Barcode2DWithSoft.ScanerPropertyNum
SCANNER_BARCODE_1D - Static variable in class com.barcode.BarcodeUtility
  1D是否已经开启
SCANNER_BARCODE_2D - Static variable in class com.barcode.BarcodeUtility
  2D是否已经开启
SCANNER_BARCODENOTREPEAT - Static variable in class com.barcode.BarcodeUtility
  条码是否重复显示
SCANNER_BROADCAST_ACTION - Static variable in class com.barcode.BarcodeUtility
  接收扫描数据的广播ACTION
SCANNER_BROADCAST_EXTRA - Static variable in class com.barcode.BarcodeUtility
  接收扫描数据的广播的extra数据
SCANNER_CONTINUOUS - Static variable in class com.barcode.BarcodeUtility
  是否是连续扫描 Whether enable continuous scan
SCANNER_CONTINUOUS_INTREVALTIME - Static variable in class com.barcode.BarcodeUtility
  连续扫描时间间隔
SCANNER_CONTINUOUSMODE - Static variable in class com.barcode.BarcodeUtility
  是否启用了连续扫描模式
SCANNER_CONTINUOUSTIMEOUT - Static variable in class com.barcode.BarcodeUtility
  连续扫描超时时间 continuous scanning overtime duration
SCANNER_ENDINDEX - Static variable in class com.barcode.BarcodeUtility
  后面去掉多少个字符
SCANNER_ENTER - Static variable in class com.barcode.BarcodeUtility
  是否启用回车
SCANNER_FAILUREBROADCAST - Static variable in class com.barcode.BarcodeUtility
  扫描失败是否发送广播 Send broadcast when scanning failure.
SCANNER_FAILURESOUND - Static variable in class com.barcode.BarcodeUtility
  扫描失败是否播放声音 whether playing notification when scanning failure.
SCANNER_FILTERCHARS - Static variable in class com.barcode.BarcodeUtility
  条码数据需要过滤的字符串
SCANNER_FORMAT_BARCODE - Static variable in class com.barcode.BarcodeUtility
  条码格式 0: Default 1: ASCII 2:GB2312 3:UTF8 4:Unicode 10:GBK, 11:GB18030 Barcode format 0: Default 1: ASCII 2:GB2312 3:UTF8 4:Unicode 10:GBK, 11:GB18030
SCANNER_ILLUMINATIONPOWERLEVEL - Static variable in class com.barcode.BarcodeUtility
  4710 扫描头亮度等级
SCANNER_KEYBORADHELPER_OPEN - Static variable in class com.barcode.BarcodeUtility
  键盘助手总开关是否已经打开
SCANNER_OUTPUTMODE - Static variable in class com.barcode.BarcodeUtility
  数据接收方式 0:键盘模拟 1:剪切板 2:系统广播 ouput mode 0: virtual key 1: clipboard 2: broadcast
SCANNER_PREFIX - Static variable in class com.barcode.BarcodeUtility
  条码前缀 barcode prefix.
SCANNER_RELEASESCAN - Static variable in class com.barcode.BarcodeUtility
  松开扫描按键是否停止扫描 loose scanning button to stop scanning or not
SCANNER_SCANKEYCODE_1 - Static variable in class com.barcode.BarcodeUtility
  扫描按键值 scan key code.
SCANNER_SCANKEYCODE_3 - Static variable in class com.barcode.BarcodeUtility
  扫描按键值 scan key code.
SCANNER_SOUND - Static variable in class com.barcode.BarcodeUtility
  扫描成功是否播放声音
SCANNER_STARTINDEX - Static variable in class com.barcode.BarcodeUtility
  前面去掉多少个字符
SCANNER_SUFFIX - Static variable in class com.barcode.BarcodeUtility
  条码后缀 barcode suffix.
SCANNER_TAB - Static variable in class com.barcode.BarcodeUtility
  是否启用tab
SCANNER_TIMEOUT - Static variable in class com.barcode.BarcodeUtility
  扫描超时 scanning time out.
SCANNER_VIBRATE - Static variable in class com.barcode.BarcodeUtility
  是否启用震动 whether vibrating when scanning success
search(Fingerprint.BufferEnum, int, int) - Method in class com.rscja.deviceapi.Fingerprint
  检索指纹库
  Searching fingerprint database
SearchLimit - Variable in class com.hsm.barcode.DecodeOptions
  Deprecated.
  Amount of time decoder will spend searching for a barcode
send(byte[]) - Method in class com.rscja.deviceapi.Infrared
  发送数据
  send Data
send(byte[]) - Method in class com.rscja.deviceapi.Module
  发送数据
  Send data
sendActiveFile(byte, byte[], byte[], byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  向安全模块发送激活文件
sendAndReceive(byte[], byte[]) - Method in class com.rscja.deviceapi.Module
  收发数据
sendAndReceiveData(byte[], byte[]) - Method in class com.rscja.deviceapi.Printer
  收发数据
  sent/received data
sendAndReceiveData(byte[], int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  (备注:禁止使用)
sendAuthData(byte[], byte[], byte[], byte[], byte[], byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  向安全模块发送认证数据
sendBusCMD(char[], char[], int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  /** 墨西哥公交命令
  Mexico bus commande
sendCommand(String) - Method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  CPU卡 T=CL发送COS指令
  CPU card T=CL send COS command
sendCommand(String) - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  CPU卡 T=CL发送COS指令
  CPU card T=CL send COS command
sendData(byte[]) - Method in class com.rscja.deviceapi.Printer
  发送数据到串口
  send data to serial port
sendData(byte[], int) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  (备注:禁止使用)
sendUserInfo(byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  向安全模块发送 用户信息数据
setAFI(String) - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  设置AFI值
  setup AFI value
setAnimalFlag(long) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置动物标签的AnimalFlag
  setup AnimalFlag of animal tag
setBarcodeEncodingFormat(Context, int) - Method in class com.barcode.BarcodeUtility
  设置条码编码格式 Setup barcode coding format
setBarcodeHeight(int) - Method in class com.rscja.deviceapi.Printer
  设置一维条码的高度
  Setup 1D barcode height
setBarcodeHRI(int) - Method in class com.rscja.deviceapi.Printer
  设置一维条码可读字符（HRI）打印位置
  setup 1D barcode readable character (HRI) print position
setBarcodeWidth(int) - Method in class com.rscja.deviceapi.Printer
  设置一维条码的宽度
  Setup 1D barcode width
setBaudrate(int) - Method in class com.rscja.deviceapi.DeviceConfiguration
  设置波特率
  Setup baudrate
setBluetoothMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  设置uhf通信方式
SetCamera_ID(int) - Method in class com.hsm.barcode.HalInterface
setClosePort() - Method in class com.rscja.deviceapi.BDNavigation
  关闭串口
  close serial port
setCodeTypeOnAndOff_IA400S(Barcode2DWithSoft.CODETYPE, boolean) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  只支持擎亚扫描头
setContinuousScanIntervalTime(Context, int) - Method in class com.barcode.BarcodeUtility
  设置连续扫描间隔时间 Setup continuous scanning duration
setContinuousScanTimeOut(Context, int) - Method in class com.barcode.BarcodeUtility
  设置连续扫描超时时间 Setup continuous scanning overtime duration
setCountryID(long) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置动物标签的国家代码
  setup national code of animal tag
setData(String) - Method in class com.rscja.deviceapi.entity.DESFireFile
  设置数据，仅对数据文件类型有效
  setup data, it is valid for value file type only
setData(String) - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  设置标签数据
  setup tag data
setDataBlock(long) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置动物标签的DataBlock
  setup DataBlock of animal tag
setDebug(boolean) - Static method in class com.rscja.utility.StringUtility
setDecodeAttemptLimit(int) - Method in class com.hsm.barcode.Decoder
  Sets the decode attempt limit (or the amount of time it will spend decoding a particular image).
setDecodeOptions(DecodeOptions) - Method in class com.hsm.barcode.Decoder
  Sets the decode options parameters.
setDecoderListeners(DecoderListener) - Method in class com.hsm.barcode.Decoder
  Used to register the listeners
setDecodeWindow(DecodeWindowing.DecodeWindow) - Method in class com.hsm.barcode.Decoder
  Sets the decode window parameters.
setDecodeWindowMode(int) - Method in class com.hsm.barcode.Decoder
  Sets the decode window mode to be used.
setDefaultParameters() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  重置扫描头参数(此函数目前只支持moto扫描头)
  reset scanning module parameter(this formula supports MOTO scanning module only)
setDESFID(String) - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  设置DESFID值
  setup DESFID value
setDeviceName(String) - Method in class com.rscja.deviceapi.DeviceConfiguration
  设置设备名
  Setup device name
setDeviceName(String) - Method in class com.rscja.deviceapi.Fingerprint
  设置设备名称
  Setup device name
setEnrollCallBack(FingerprintWithFIPS.EnrollCallBack) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置采集指纹回调接口
  Setup call-back contact for acquiring fingerprint
setEPC(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setEPCTIDMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHF
  开关同时读取 EPC 和 TID 模式设置功能，仅R2000有效
  ON/OFF will read EPC and TID setup function simultaneously, it is valid for R2000 only.
setExposureMode(int) - Method in class com.hsm.barcode.Decoder
  Sets the exposure mode to be used during scanning.
setExposureSettings(int[]) - Method in class com.hsm.barcode.Decoder
  Sets the current exposure settings for the image sensor.
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHF
  开关FastID功能，仅R2000有效
  ON/OFF FastID function, R2000 is valid only.
setFeedRow(int) - Method in class com.rscja.deviceapi.Printer
  打印并进纸 n行
  print and paper infeed n
setFileSize(int) - Method in class com.rscja.deviceapi.entity.DESFireFile
  设置文件大小，仅对数据文件类型有效
  setup file size, it is valid for data file type only
setFilter(int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
setFilter(RFIDWithUHF.BankEnum, int, int, String, boolean) - Method in class com.rscja.deviceapi.RFIDWithUHF
setFilter(int, byte, String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
setFlags(int) - Method in class com.hsm.barcode.SymbologyConfig
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置模块频点
  setup frequence point module
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  设置模块频点
setFrequency(int) - Method in class com.rscja.deviceapi.RFIDWithUHF706
setFrequencyMode(byte) - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置模块的工作模式
  setup module work mode
setFrequencyMode(byte) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  设置模块的工作模式
SetGen2(int, int, int, int, int, int, int, int, int, int, int, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
setGrabCallBack(FingerprintWithFIPS.GRABCallBack) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置获取图片回调接口
  Setup call-back contact for acquiring picture
setId(String) - Method in class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
setID(String) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置指纹模块ID
  Setup fingerprint module ID
setIdData(String) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置64bit的识别号数据，十六进制表示
  setup 64bit identification number, hexdecimal
setIdentificationCallBack(FingerprintWithFIPS.IdentificationCallBack) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置指纹验证回调接口
  Setup fingerprint verification
setIdentificationCallBack(FingerprintWithMorpho.IdentificationCallBack) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置指纹验证回调接口
  setup fingerprint verification call-back contact
setInventoryBID(boolean, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  盘存TID(客户定制函数/Customizing)
SetInventorySper(int) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  开始读 flag：0 表示定频 1：表跳频
setKeyEventCallback(RFIDWithUHFBluetooth.KeyEventCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  设置接收扫描按键的回调
setKeyEventCallback(RFIDWithUHFBluetooth.KeyEventCallback) - Method in class com.rscja.deviceapi.service.BTService
setLastImage(byte[], int, int) - Method in class com.hsm.barcode.Decoder
  Sets last image that will be sent to the Decoder.
setLicense_IA400S(String) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
setLightsMode(int) - Method in class com.hsm.barcode.Decoder
  Sets the lights mode for scanning.
setLog(boolean) - Method in class com.rscja.deviceapi.CardWithBYL
setManuFacture(String) - Method in class com.rscja.deviceapi.Fingerprint
  设置厂商名称
  Setup manufacture name
setMaxLength(int) - Method in class com.hsm.barcode.SymbologyConfig
setMaxValue(int) - Method in class com.rscja.deviceapi.entity.DESFireFile
  设置最小值，仅对值文件类型有效
  setup minimum value, it is valid for value file type only
setMinLength(int) - Method in class com.hsm.barcode.SymbologyConfig
setMinValue(int) - Method in class com.rscja.deviceapi.entity.DESFireFile
  设置最小值，仅对值文件类型有效
  setup minimum value, it is valid for value file type only
setMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置寻标签模式，仅R2000模块有效
  setup tag searching mode, it is valid for R2000 only.
setMorphoLoadKs(byte[]) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置加密数据秘钥
  Setup encypted data key
setMorphoSecurityLevel(int) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
setNationalID(long) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置动物标签的NationalID信息
  setup NationalID infor of animal tag
setNoDisplayMode() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  此函数目前只支持moto扫描头
  This formula supports MOTO scanning module only
setNumber(String) - Method in class com.rscja.deviceapi.entity.SatelliteEntity
setOCRMode(int) - Method in class com.hsm.barcode.Decoder
  Sets the OCR Mode (used for enabling/disabling)
setOCRTemplates(int) - Method in class com.hsm.barcode.Decoder
  Sets the OCR template configuration (pre-defined).
setOCRUserTemplate(byte[]) - Method in class com.hsm.barcode.Decoder
  Sets the OCR User defined template.
setOpenPort() - Method in class com.rscja.deviceapi.BDNavigation
  打开串口
  open serial port
setOriginalUID(char[]) - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  设置标签原始的UID
  setup original UID of tag
setOutputMode(Context, int) - Method in class com.barcode.BarcodeUtility
  设置输出模式 Setup ouput mode
SetPackageName(String) - Method in class com.hsm.barcode.HalInterface
setPara(int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  设置参数
setParam(char, char[], char[]) - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置模块参数，仅R2000模块有效
  setup module parameter, it is valid for R2000 only
setParam_zebra(Context, int, int) - Method in class com.barcode.BarcodeUtility
  设置斑马扫描头参数,扫描头上电之后设置一次即可,扫描头断电之后失效。(备注：键盘助手v2.2.0.3 之后的版本才支持)
setParameter(int, int) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  设置扫描头参数(此函数目前只支持moto扫描头)
  Setup scanning module parameter( this formula supports MOTO scanning module only)
setParameter(int, String) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  设置扫描头参数(此函数目前只支持moto扫描头)
setPower(int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置模块的功率
  setup module power
setPower(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  两个字节长度的功率
setPower(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  设置模块的功率
setPrefix(Context, String) - Method in class com.barcode.BarcodeUtility
  设置前缀 Setup prefix
setPreviewDisplay(SurfaceHolder) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  设置预览控件(只支持mot扫描头)
  setup preview control( supports MOTO scanning module only.)
setPrintCharacterStyle(boolean, boolean, boolean, boolean, boolean, boolean, boolean) - Method in class com.rscja.deviceapi.Printer
  设置字体样式
  set font style
setPrinterStatusCallBack(Printer.PrinterStatusCallBack) - Method in class com.rscja.deviceapi.Printer
  设置接收打印机状态的回调
  set call back of printer received status
setPrinterStatusCallBackEnable(boolean) - Method in class com.rscja.deviceapi.Printer
  设置是否接收打印机状态回调消息
  Setup receive printer status return message or not
setPrintGrayLevel(int) - Method in class com.rscja.deviceapi.Printer
  设置打印 灰度
  setup print grey level
setPrintLeftMargin(int) - Method in class com.rscja.deviceapi.Printer
  设置左边距
  Setup left margin
setPrintRightMargin(int) - Method in class com.rscja.deviceapi.Printer
  设置左边距
  Setup right margin
setPrintRowSpacing(int) - Method in class com.rscja.deviceapi.Printer
  设置行间距(若设定的行间距小于一行中的最大字符高度，那么该行行间距等于最大字符高度)
  Setup line spacing (if the set value is less than max.charater height, then the line spacing equals to max.character height)
setPrintSpeed(int) - Method in class com.rscja.deviceapi.Printer
  设置打印速度
  setup print velocity
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置协议 仅R2000模块有效
  setup protocol, be valid for R2000 module only
setPtCaptureCallBack(FingerprintWithFIPS.PtCaptureCallBack) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置获取指纹模版回调接口
  Setup call-back contact for acquiring fingerprint template
setPtCaptureCallBack(FingerprintWithMorpho.PtCaptureCallBack) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置获取指纹模版回调接口
  Setup call-back contact for acquiring fingerprint template
setPtEnrollCallBack(FingerprintWithMorpho.EnrollCallBack) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置采集指纹回调接口
  setup fingerprint acquire call-back contact
setPWD(String) - Method in class com.rscja.deviceapi.Fingerprint
  设置密码
  Setup password
setPwm(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置占空比，仅适用于R2000模块
  setup duty ration, used for R2000 module
setQTPara(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHF
  开启寻隐藏区(仅R2000 QT标签)
  activate searching hidden area (R2000 QT tag only)
setRawData(String) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置原始数据
  setup original data
setReadMode(RFIDWithUHF.SingleModeEnum) - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置读取模式
  setup reading mode
setReg(int, int) - Method in class com.rscja.deviceapi.Fingerprint
  设置寄存器值，修改模块参数
  Setup the value in RAM, modify the parameter in module.
setReleaseScan(Context, boolean) - Method in class com.barcode.BarcodeUtility
  松开扫描按键是否停止扫描 loose scanning button to stop scanning or not
setReserved(long) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置动物标签的Reserved信息
  setup Reserved infor of animal tag
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置链路参数，仅R2000有效
  setup link parameter, R2000 is valid only
setRTC(long) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  设置RTC时间
setScanCallback(Barcode2DWithSoft.ScanCallback) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  设置回调对象接收条码数据
  Setup call-back target to acquire barcode data.
setScanFailureBroadcast(Context, boolean) - Method in class com.barcode.BarcodeUtility
  扫描失败是否发送广播 Send broadcast when scanning failure.
setScanOutTime(Context, int) - Method in class com.barcode.BarcodeUtility
  设置超时时间 Setup overtime duration
setScanResultBroadcast(Context, String, String) - Method in class com.barcode.BarcodeUtility
  设置接收扫描数据的广播 Setup broad cast of received scanning data
setShowDecodeWindow(int) - Method in class com.hsm.barcode.Decoder
  Sets the show decode window setting.
setSignal(String) - Method in class com.rscja.deviceapi.entity.SatelliteEntity
setSuffix(Context, String) - Method in class com.barcode.BarcodeUtility
  设置后缀 Setup suffix
setSymbologyConfig(SymbologyConfig) - Method in class com.hsm.barcode.Decoder
  Sets the current configuration of the passed in structure.
setSymbologyDefaults(int) - Method in class com.hsm.barcode.Decoder
  Sets the passed in symbology ID defaults.
SetSymbologySettings(Decoder, SymbologyConfiguration.BarcodeSymbologyID, SymbologyConfig) - Method in class com.zebra.adc.decoder.SymbologyConfiguration
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHF
  开关TagFocus功能，仅R2000有效
  ON/OFF TagFocus function, it is valid for R2000 only.
setTemplateVerifyCallBack(FingerprintWithFIPS.TemplateVerifyCallBack) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置模版比对回调接口
  Setup call-back contact for template comparison
setTemplateVerifyCallBack(FingerprintWithMorpho.TemplateVerifyCallBack) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置模版比对回调接口
  Setup call-back contact for template comparison
SetTestMode() - Method in class com.rscja.deviceapi.RFIDWithUHF706
  设置为测试模式
setTimeOut(int) - Method in class com.rscja.deviceapi.Barcode1D
  设置超时时间
  set time out.
setTimeOut(int) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
setTimeOut(int) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  设置超时时间
  setup time-out duration
setUart(String) - Method in class com.rscja.deviceapi.DeviceConfiguration
  设置串口路径
  Setup serial port directory.
setUart(String) - Method in class com.rscja.deviceapi.RFIDWithUHF
  设置uhf串口，成为的手持机不要调用此函数，否则uhf会无法工作
setVersions(String) - Method in class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
setWorkMode(int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHF706
  设置安全模块的工作模式
SimpleRFIDEntity - Class in com.rscja.deviceapi.entity
  RFID简单数据实体
  RFID simple data entity
SimpleRFIDEntity(String, String) - Constructor for class com.rscja.deviceapi.entity.SimpleRFIDEntity
  构造函数
  create formula
SimpleRFIDEntity(String, String, byte[]) - Constructor for class com.rscja.deviceapi.entity.SimpleRFIDEntity
  构造函数
  create formula
Size - Variable in class com.hsm.barcode.ImagerProperties
  Size of this structure
SPECIAL - Static variable in class com.hsm.barcode.ExposureValues.SpecularExclusion
  Deprecated.
  Do not use
SpecularExclusion() - Constructor for class com.hsm.barcode.ExposureValues.SpecularExclusion
  Deprecated.
startBTScan(RFIDWithUHFBluetooth.ScanBTCallback) - Method in class com.rscja.deviceapi.service.BTService
startEnroll() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  开始采集指纹,注意:请调用
  start acquire fingerprint, attention: call out
  `FingerprintWithFIPS.setEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithFIPS.setEnrollCallBack(EnrollCallBack callBack)`setup receviced call-back data
startEnroll(int, String) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始采集指纹,注意:请调用
  Start acquire fingerprint, attention: call out
  `FingerprintWithMorpho.setPtEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setPtEnrollCallBack(EnrollCallBack callBack)` setup receive call-back data
startGRAB() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  开始获取图片,注意:请调用
  start acquire picture, attention: call out
  `FingerprintWithFIPS.setGrabCallBack(GRABCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithFIPS.setGrabCallBack(GRABCallBack callBack)`method to setup received call-back data.
startHandsFree() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  设置连续扫描(只支持moto扫描头)
  Setup continuous scanning function(supports MOTO scanning module only)
startIdentification() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  开始验证指纹,注意:请调用
  start verify finerprint, attention: call out
  `FingerprintWithFIPS.setIdentificationCallBack(IdentificationCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithFIPS.setIdentificationCallBack(IdentificationCallBack callBack)` setup receviced call-back data
startIdentification() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始验证指纹,注意:请调用
  Start verify fingerprint, attention: call-out
  `FingerprintWithMorpho.setIdentificationCallBack(IdentificationCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setIdentificationCallBack(IdentificationCallBack callBack)` setup receive call-back data
startInventory(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  Deprecated.
startInventory_BankPtrCnt(int, int, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  客户定制
  Customizing
startInventoryTag(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  启动识别Tag循环，只是开启识别Tag循环，之后将识别到的标签号上传到缓冲区， `RFIDWithUHF.readTagFromBuffer()`
  activate identification Tag circulation, upload the identified tag number to buffer zone after, `RFIDWithUHF.readTagFromBuffer()`
  用于从缓冲区读取一个标签号数据，开启循环识别之后，模块只能响应`RFIDWithUHF.stopInventory()` 函数， used for reading one tag data, after starting the circular identification, the module will respond `RFIDWithUHF.stopInventory()` formula.
  `RFIDWithUHF.stopInventory()` 停止识别循环。
  `RFIDWithUHF.stopInventory()` stop identification circulation.
startInventoryTag(int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHF
  启动识别Tag循环，只是开启识别Tag循环，之后将识别到的标签号上传到缓冲区， `RFIDWithUHF.readTagFromBuffer()`
  start identifing Tag circulation, start identifying Tag circulation only, upload the identified tag number to buffer zone after, `RFIDWithUHF.readTagFromBuffer()`
  用于从缓冲区读取一个标签号数据，开启循环识别之后，模块只能响应`RFIDWithUHF.stopInventory()` 函数，
  used for reading a tag number data from buffer zone, after starting circular identification, module will respond `RFIDWithUHF.stopInventory()` formula only.
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  开始循环识别
startPreview() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  启动预览(只支持mot扫描头)
  activate preview(suppots MOTO scanning module only)
startPtCapture() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call up
  `FingerprintWithFIPS.setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithFIPS.setPtCaptureCallBack(PtCaptureCallBack callBack)` method to setup received call-back data.
startPtCapture(boolean) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call out
  `FingerprintWithMorpho.setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setPtCaptureCallBack(PtCaptureCallBack callBack)` setup receive call-back data
startPtCapturePKComp(boolean) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call out
  `FingerprintWithMorpho.setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setPtCaptureCallBack(PtCaptureCallBack callBack)` setup receive call-back data
startScan(Context, BarcodeUtility.ModuleType) - Method in class com.barcode.BarcodeUtility
  开始扫描 Start scanning
startScanning() - Method in class com.hsm.barcode.Decoder
  Starts scanning operation (image taking, not decoding).
startTemplateVerify(char[]) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  开始模版验证,注意:请调用
  start template verification, attention: call out
  `FingerprintWithFIPS.setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithFIPS.setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)`method to setup received call-back data.
startTemplateVerify(byte[], int) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始模版验证,注意:请调用
  start template verification, attention: call out
  `FingerprintWithMorpho.setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)`method to setup received call-back data.
startViewFinder(Barcode2DWithSoft.VideoCallback) - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  开始捕捉帧视频模式(只支持mot扫描头)
  Start capture frame vedio mode(support MOTO scanning module only)
stopEnroll() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  停止采集指纹
  Stop acquiring fingerprint
stopGRAB() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  停止获取图片
  stop acquiring picture
stopHandsFree() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  停止连续扫描(只支持moto扫描头)
  Stop continuous scanning (support MOTO scanning module)
stopIdentification() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  停止指纹验证
  Stop fingerprint verification
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHF
  停止循环识别
  stop circular identification
stopInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  停止循环识别
stopPreview() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  停止预览(只支持mot扫描头)
  Stop preview(supports MOTO scanning module only)
stopPtCapture() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  停止获取指纹模版
  Stop acquiring fingerprint template
stopScan(Context, BarcodeUtility.ModuleType) - Method in class com.barcode.BarcodeUtility
  停止扫描 Stop scanning
stopScan() - Method in class com.rscja.deviceapi.Barcode1D
  终止扫描
  Scanning terminated
stopScan() - Method in class com.rscja.deviceapi.Barcode2D
  终止扫描
  Scanning terminated
stopScan() - Method in class com.zebra.adc.decoder.Barcode2DWithSoft
  终止扫描
  Scanning terminated
stopScanBTDevices() - Method in class com.rscja.deviceapi.RFIDWithUHFBluetooth
  停止扫描蓝牙设备
stopScanning() - Method in class com.hsm.barcode.Decoder
  Stops scanning operation (image taking, not decoding).
stoptBTScan() - Method in class com.rscja.deviceapi.service.BTService
stopTemplateVerify() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  停止模版比对
  Stop template comparison
storChar(Fingerprint.BufferEnum, int) - Method in class com.rscja.deviceapi.Fingerprint
  存储模板文件。将模板缓冲区buffer中的模板文件存到 PageID号所对应的指纹库位置
  save templatefile.
string2Int(String, int) - Static method in class com.rscja.utility.StringUtility
  字符串转整数
StringUtility - Class in com.rscja.utility
  字符工具类
StringUtility() - Constructor for class com.rscja.utility.StringUtility
switchBaudrate(int, int, int, int) - Method in class com.rscja.deviceapi.Infrared
  切换波特率
SYM_ALL - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  All Symbologies
SYM_AUSPOST - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Australian Post [2D Postal]
SYM_AZTEC - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Aztec Code
SYM_BPO - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  British Post [2D Postal]
SYM_CANPOST - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Canadian Post [2D Postal]
SYM_CHINAPOST - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  China Post
SYM_CODABAR - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Codabar
SYM_CODABLOCK - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Codablock F
SYM_CODE11 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Code 11
SYM_CODE128 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Code 128
SYM_CODE16K - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Deprecated.
  Code 16K
SYM_CODE32 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Code 32 Italian Pharmacy Code
SYM_CODE39 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Code 39
SYM_CODE49 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Deprecated.
  Code49
SYM_CODE93 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Code 93
SYM_COMPOSITE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  EAN UCC Composite
SYM_COUPONCODE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Coupon Code
SYM_DATAMATRIX - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Data Matrix
SYM_DUTCHPOST - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  KIX (Netherlands) Post [2D Postal]
SYM_EAN13 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  EAN-13
SYM_EAN8 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  EAN-8
SYM_GRIDMATRIX - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Grid Matrix
SYM_GS1_128 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  GS1 128
SYM_HANXIN - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Hanxin
SYM_IATA25 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Straight 2 of 5 IATA (two-bar start/stop)
SYM_IDTAG - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  UPU 4 State [2D Postal]
SYM_INT25 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Interleaved 2 of 5
SYM_ISBT - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  ISBT 128
SYM_JAPOST - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Japanese Post [2D Postal]
SYM_KOREAPOST - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Korean Post
SYM_LABEL - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Deprecated.
  Label
SYM_MASK_ALL - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  All fields valid
SYM_MASK_FLAGS - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Flags are valid
SYM_MASK_MAX_LEN - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Max Length valid
SYM_MASK_MIN_LEN - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Min Length valid
SYM_MATRIX25 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Matrix 2 of 5
SYM_MAXICODE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Maxicode
SYM_MICROPDF - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Micro PDF
SYM_MSI - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  MSI
SYM_OCR - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Deprecated.
  OCR
SYM_PDF417 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  PDF417
SYM_PLANET - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Planet Code [2D Postal]
SYM_PLESSEY - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Deprecated.
  Plessey Code
SYM_POSICODE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Deprecated.
  Posicode
SYM_POSTALS - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Used to default and disable postal codes
SYM_POSTNET - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Deprecated.
  Postnet
SYM_QR - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  QR Code
SYM_RSS - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Reduced Space Symbology (RSS-14, RSS Limited, RSS Expanded)
SYM_STRT25 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Straight 2 of 5 Industrial (three-bar start/stop)
SYM_TELEPEN - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Telepen
SYM_TLCODE39 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  TCIF Linked Code 39 (TLC39)
SYM_TRIOPTIC - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Trioptic Code
SYM_UPCA - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  UPC-A
SYM_UPCE0 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  UPC-E0
SYM_UPCE1 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  UPC-E1
SYM_US_POSTALS1 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Used to enable SYM_PLANET, SYM_POSTNET, SYM_USPS4CB & SYM_IDTAG
SYM_USPS4CB - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  USPS 4 State (Intelligent Mail Barcode) [2D Postal]
SYMBOLOGIES - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyID
  Number of Symbologies
SYMBOLOGY_128_APPEND - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Deprecated.
  Enable OR dISBALE Code 128 FNC2 append functionality
SYMBOLOGY_2_DIGIT_ADDENDA - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Enable 2 digit Addenda (UPC & EAN)
SYMBOLOGY_5_DIGIT_ADDENDA - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Enable 5 digit Addenda (UPC & EAN)
SYMBOLOGY_ADDENDA_REQUIRED - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Only allow codes with addenda (UPC & EAN)
SYMBOLOGY_ADDENDA_SEPARATOR - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Include Addenda separator space in returned string
SYMBOLOGY_AUS_POST_ALPHANUMERIC_C_TABLE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Alphanumeric C Table
SYMBOLOGY_AUS_POST_COMBINATION_N_AND_C_TABLES - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Combination N and C Tables
SYMBOLOGY_AUS_POST_NUMERIC_N_TABLE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Numeric N Table
SYMBOLOGY_AUSTRALIAN_BAR_WIDTH - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Include australian postal bar data in string
SYMBOLOGY_CHECK_ENABLE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Enable usage of check character
SYMBOLOGY_CHECK_TRANSMIT - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Send check character
SYMBOLOGY_CODABAR_CONCATENATE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Codabar concatenate.
SYMBOLOGY_COMPOSITE_UPC - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Enable UPC composite codes
SYMBOLOGY_ENABLE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Enable Symbology bit
SYMBOLOGY_ENABLE_APPEND_MODE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Deprecated.
  Code39 append mode
SYMBOLOGY_ENABLE_FULLASCII - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Enable Code39 Full ASCII
SYMBOLOGY_EXPANDED_UPCE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Extended UPC-E
SYMBOLOGY_NUM_SYS_TRANSMIT - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  UPC-A/UPC-e Send Num Sys
SYMBOLOGY_POSICODE_LIMITED_1 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Deprecated.
  PosiCode Limited of 1
SYMBOLOGY_POSICODE_LIMITED_2 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Deprecated.
  PosiCode Limited of 2
SYMBOLOGY_RSE_ENABLE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Enable RSS Expanded bit
SYMBOLOGY_RSL_ENABLE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Enable RSS Limited bit
SYMBOLOGY_RSS_ENABLE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Enable RSS bit
SYMBOLOGY_RSX_ENABLE_MASK - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Enable all RSS versions
SYMBOLOGY_START_STOP_XMIT - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Include the start and stop characters in the decoded result string
SYMBOLOGY_TELEPEN_OLD_STYLE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Telepen Old Style mode
SYMBOLOGY_UPCA_TRANSLATE_TO_EAN13 - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  Translate UPCA to EAN13 if EAN 13 and UPC are enabled
SYMBOLOGY_UPCE1_ENABLE - Static variable in class com.hsm.barcode.DecoderConfigValues.SymbologyFlags
  UPC-E1 enable (use SYMBOLOGY_ENABLE for UPC-E0)
SymbologyConfig - Class in com.hsm.barcode
  Symbology configuration for setting symbology settings.
SymbologyConfig() - Constructor for class com.hsm.barcode.SymbologyConfig
SymbologyConfiguration - Class in com.zebra.adc.decoder
SymbologyConfiguration() - Constructor for class com.zebra.adc.decoder.SymbologyConfiguration
SymbologyConfiguration.BarcodeSymbologyID - Enum in com.zebra.adc.decoder
symID - Variable in class com.hsm.barcode.SymbologyConfig
  Symbology ID

A B C D E F G H I K L M N O P R S T U V W X Y