Deprecated List

# Deprecated API

## Contents

- Deprecated Classes
- Deprecated Enums
- Deprecated Fields
- Deprecated Methods

- Deprecated Classes
  Class and Description
  com.hsm.barcode.ExposureValues.ExposureMethod ExposureMethod class that defines the auto exposure method that will be used during image capture.
  com.hsm.barcode.ExposureValues.SpecularExclusion SpecularExclusion class that defines the specular exclusion setting in the ExposureSettings class that will be used during image capture.

- Deprecated Enums
  Enum and Description
  com.rscja.deviceapi.RFIDWithUHF.LockModeEnum

- Deprecated Fields
  Field and Description
  com.hsm.barcode.DecodeOptions.CallbackWaitTimeout Timeout setting decWaitForDecode will wait before checking callback (WinCE Only)
  com.hsm.barcode.ExposureValues.ExposureSettings.DEC_ES_EXPOSURE_METHOD Exposure method to use
  com.hsm.barcode.ExposureValues.ExposureSettings.DEC_ES_FRAME_RATE Frame rate to use - fixed cannot be changed
  com.hsm.barcode.ExposureValues.ExposureSettings.DEC_ES_SPECULAR_EXCLUSION Specular exclusion value to use
  com.hsm.barcode.ExposureValues.ExposureSettings.DEC_ES_SPECULAR_LIMIT If specular exclusion is set, what is the limit
  com.hsm.barcode.ExposureValues.ExposureSettings.DEC_ES_SPECULAR_SAT If specular exclusion is set, what is the saturation value
  com.hsm.barcode.ExposureValues.ExposureSettingsMinMax.DEC_MAX_ES_EXPOSURE_METHOD Maximum exposure method setting
  com.hsm.barcode.ExposureValues.ExposureSettingsMinMax.DEC_MAX_ES_FRAME_RATE Maximum frame rate setting
  com.hsm.barcode.ExposureValues.ExposureSettingsMinMax.DEC_MAX_ES_SPECULAR_EXCLUSION Maximum specular exclusion setting
  com.hsm.barcode.ExposureValues.ExposureSettingsMinMax.DEC_MAX_ES_SPECULAR_LIMIT Maximum specular limit setting
  com.hsm.barcode.ExposureValues.ExposureSettingsMinMax.DEC_MAX_ES_SPECULAR_SAT Maximum specular saturation setting
  com.hsm.barcode.ExposureValues.ExposureSettingsMinMax.DEC_MIN_ES_EXPOSURE_METHOD Minimum exposure method setting
  com.hsm.barcode.ExposureValues.ExposureSettingsMinMax.DEC_MIN_ES_FRAME_RATE Minimum frame rate setting
  com.hsm.barcode.ExposureValues.ExposureSettingsMinMax.DEC_MIN_ES_SPECULAR_EXCLUSION Minimum specular exclusion setting
  com.hsm.barcode.ExposureValues.ExposureSettingsMinMax.DEC_MIN_ES_SPECULAR_LIMIT Minimum specular limit setting
  com.hsm.barcode.ExposureValues.ExposureSettingsMinMax.DEC_MIN_ES_SPECULAR_SAT Minimum specular saturation setting
  com.hsm.barcode.DecodeOptions.DecodeMode Decoding modes
  com.hsm.barcode.ImageAttributes.IlluminationClipValue Illumination clip value
  com.hsm.barcode.DecoderConfigValues.EngineID.IMAGER_4200_ENGINE 4200 Engine ID
  com.hsm.barcode.DecoderConfigValues.EngineID.IMAGER_IT4000_ENGINE IT4000 Engine ID
  com.hsm.barcode.DecoderConfigValues.EngineID.IMAGER_IT4100_ENGINE IT4100 Engine ID
  com.hsm.barcode.DecoderConfigValues.EngineID.IMAGER_IT4300_ENGINE IT4300 Engine ID
  com.hsm.barcode.DecoderConfigValues.EngineID.LASER_SE1200_ENGINE SE1200 Laser Engine ID
  com.hsm.barcode.DecoderConfigValues.EngineID.LASER_SE1223_ENGINE SE1223 Laser Engine ID
  com.hsm.barcode.DecodeOptions.LinearRange Size of the window used in the Advanced Linear decoding mode
  com.hsm.barcode.DecodeOptions.PrintWeight Relative contrast
  com.hsm.barcode.DecodeOptions.SearchLimit Amount of time decoder will spend searching for a barcode
  com.hsm.barcode.DecoderConfigValues.SymbologyID.SYM_CODE16K Code 16K
  com.hsm.barcode.DecoderConfigValues.SymbologyID.SYM_CODE49 Code49
  com.hsm.barcode.DecoderConfigValues.SymbologyID.SYM_LABEL Label
  com.hsm.barcode.DecoderConfigValues.SymbologyID.SYM_OCR OCR
  com.hsm.barcode.DecoderConfigValues.SymbologyID.SYM_PLESSEY Plessey Code
  com.hsm.barcode.DecoderConfigValues.SymbologyID.SYM_POSICODE Posicode
  com.hsm.barcode.DecoderConfigValues.SymbologyID.SYM_POSTNET Postnet
  com.hsm.barcode.DecoderConfigValues.SymbologyFlags.SYMBOLOGY_128_APPEND Enable OR dISBALE Code 128 FNC2 append functionality
  com.hsm.barcode.DecoderConfigValues.SymbologyFlags.SYMBOLOGY_ENABLE_APPEND_MODE Code39 append mode
  com.hsm.barcode.DecoderConfigValues.SymbologyFlags.SYMBOLOGY_POSICODE_LIMITED_1 PosiCode Limited of 1
  com.hsm.barcode.DecoderConfigValues.SymbologyFlags.SYMBOLOGY_POSICODE_LIMITED_2 PosiCode Limited of 2

- Deprecated Methods
  Method and Description
  com.rscja.deviceapi.FingerprintWithFIPS.decryption(byte[], int)
  com.rscja.deviceapi.FingerprintWithFIPS.decryption(byte[], int, byte[])
  com.rscja.deviceapi.FingerprintWithFIPS.decryption(byte[], int, String)
  com.rscja.deviceapi.FingerprintWithFIPS.Encryption(byte[], int)
  com.rscja.deviceapi.FingerprintWithFIPS.Encryption(byte[], int, String)
  com.rscja.deviceapi.RFIDWithUHF.generateLockCode(RFIDWithUHF.LockModeEnum, RFIDWithUHF.LockModeEnum, RFIDWithUHF.LockModeEnum, RFIDWithUHF.LockModeEnum, RFIDWithUHF.LockModeEnum)
  com.hsm.barcode.Decoder.getDecThreadsRevision() Retrieves the revision of the Decoder Threading.
  com.hsm.barcode.Decoder.getSecondaryDecoderRevision() Secondary Decoder currently unsupported
  com.rscja.deviceapi.RFIDWithUHF.init_R2000()
  com.rscja.deviceapi.RFIDWithUHF.inventorySingleTagWithR2000()
  com.rscja.utility.StringUtility.isHexNumber(String)
  com.rscja.deviceapi.RFIDWithUHF.killTag(String)
  com.rscja.deviceapi.RFIDWithUHF.lockMem(String, String)
  com.rscja.deviceapi.RFIDWithUHF.lockMem(String, String, String)
  com.rscja.deviceapi.RFIDWithUHF.openInventoryEPCAndTIDMode()
  com.rscja.deviceapi.RFIDWithUHF.readData(String, RFIDWithUHF.BankEnum, int, int, String)
  com.rscja.deviceapi.RFIDWithUHF.readDataWithQT(String, RFIDWithUHF.BankEnum, int, int, String)
  com.rscja.deviceapi.RFIDWithUHF.readTagFromR2000Buffer()
  com.rscja.deviceapi.RFIDWithUHF.setFilter(int, byte, String)
  com.rscja.deviceapi.RFIDWithUHF.setFilter(int, int, String)
  com.rscja.deviceapi.RFIDWithUHF.startInventory(int, int)
  com.rscja.deviceapi.Module.uartSwitch2(int)
  com.rscja.deviceapi.RFIDWithUHF.writeData(String, RFIDWithUHF.BankEnum, int, int, String)
  com.rscja.deviceapi.RFIDWithUHF.writeData(String, RFIDWithUHF.BankEnum, int, int, String, String)
  com.rscja.deviceapi.RFIDWithUHF.writeDataWithQT(String, RFIDWithUHF.BankEnum, int, int, String)
  com.rscja.deviceapi.RFIDWithUHF.writeDataWithQT(String, RFIDWithUHF.BankEnum, int, int, String, String)